>> MIB - Management Information Base
>> Table: vlanMemberTable - (.1.3.6.1.4.1.272.4.39.3.1)
Description: Each entry contains a unique virtIfIndex and the physical address used. The corresponding IP-Address musr be taken from the ipAddressTable.
vlanMemberTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | VlanId | INTEGER | RW
.3 | Egress | ENUM | RW
.4 | Status | ENUM | D
IfIndex
Interface Index of the VLAN Member.
VlanId
VLAN Id of the VLAN member. Range: 0 to 4095
Egress
Selects how frames will egress the interface. Enumerations: untagged (1) tagged (2) drop (3)
Status
Status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH