>> MIB - Management Information Base
>> Table: biboAdmSyslogTable - (.1.3.6.1.4.1.272.4.1.12.1)
Description: The biboAdmSyslogTable keeps track of syslog messages received. The size of the table (number of entries), is limited by the value of biboAdmSyslogMaxEntries. The columns specify attributes for each message generated. As this information only reports events on the system, all fields are read-only. Creating entries: Entries can only be created by the system and are made each time a syslog message is generated. Deleting entries: Entries are removed by the system once the size limit (biboAdmSyslogMaxEntries) is reached.
biboAdmSyslogTable
OID | Name | Type | Access
.1 | TimeStamp | Date | R
.2 | Level | ENUM | R
.4 | Message | DisplayString | R
.5 | Subject | ENUM | R
TimeStamp
Time message was generated. Range: 0 to -1
Level
Level of syslog message. Enumerations: emerg (1) alert (2) crit (3) err (4) warning (5) notice (6) info (7) debug (8)
Message
The text of the syslog message. Length: 0 to 255
Subject
Subject of the syslog message. Enumerations: acct (1) isdn (2) inet (3) x25 (4) ipx (5) capi (6) ppp (7) bridge (8) config (9) snmp (10) x21 (11) token (12) ether (13) radius (14) tapi (15) ospf (16) fr (17) modem (18) rip (19) atm (20) pabx (21) ipsec (22) tty (23) bgp (24) tacacs (25) brrp (26) mps (27) voip (28) tr069 (29) wlan (30) usb (31) http (32) inet6 (33) wlc (34) ldap (35) osp (36) wtp (37) tremp (38) presence (39)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH