>> MIB - Management Information Base
>> Table: ip6AddrTable - (.1.3.6.1.4.1.272.4.5.100.2.4.1)
Description: List of own interface-addresses currently used by this node.
ip6AddrTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RC
.2 | Prefix | Unsigned32 | R
.3 | Length | INTEGER | R
.4 | Address | InetAddressIPv6 | R
.5 | Scope | ENUM | R
.6 | Type | ENUM | R
.7 | LkPrefix | Unsigned32 | R
IfIndex
ip6IfIndex of related interface. Range: 1 to 2147483647
Prefix
ip6PrefixId of related ip6Prefix-entry, if any, else 0.
Length
Length of related prefix. Range: 1 to 128
Address
Address-value. Length: 16 to 16
Scope
Scope of this address. Enumerations: linklocal (2) global (14)
Type
'Type' of this address. stateless(1) - Auto-configured (see RFC-4862). stateful(2) - Learned from DHCPv6-server. static(3) - Configured via ip6AdmAddr-entry. anycast(4) - Dummy-entry for anycast-receipt. unknown(5) - Used for debugging only. Enumerations: stateless (1) stateful (2) static (3) anycast (4) unknown (5)
LkPrefix
ip6LinkPrefixId of related ip6LinkPrefix-entry, if any, else 0.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH