>> MIB - Management Information Base
>> Table: ipTdrcTable - (.1.3.6.1.4.1.272.4.5.43.1)
Description: The ipTdrcTable enables the TCP Download Rate Control (TDRC) on the interface specified by ipTdrcIfIndex (interface index). Creating entries: Entries are created by assigning an interface index to the ipTdrcIfIndex object. Deleting entries: Entries are removed by setting an entry's ipTdrcMode object to 'delete'.
ipTdrcTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Mode | ENUM | D
.3 | MaxRate | INTEGER | RW
.4 | WindowScaling | INTEGER | RW
.5 | Mss | INTEGER | RW
.6 | Services | ENUM | RW
IfIndex
The associated Interface Index.
Mode
The TDRC mode for the associated interface. disabled(1): no TDRC active ack-prioritisation(2): preferential transmission of TCP ACK messages static(3): static TCP download limitation determined by ipTdrcMaxRate dynamic(4): dynamic TCP download limitation determined by ipTdrcMaxRate less amount of high priority traffic send via the associated interface delete(5): this entry will be deleted Enumerations: disabled (1) ack-prioritisation (2) static (3) dynamic (4) delete (5)
MaxRate
The maximum TCP download rate in bits per second.
WindowScaling
The TCP window scaling used for TDRC. Range: 0 to 16
Mss
The TCP MSS used for TDRC. Range: 0 to 4056
Services
Determines the TCP services to be considered for TDRC. If set to listed-only(1), only the predefined and listed services (see ipTdrcServiceTable) will be controlled. If set to all(2) each TCP service will be controlled. Enumerations: listed-only (1) all (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH