>> MIB - Management Information Base
>> Table: ipPublishTable - (.1.3.6.1.4.1.272.4.5.24.1)
Description: This entry contains all data for managing one dynamic DNS account hosted by a provider which is defined in one entry of the ipDynDnsProviderTable.
ipPublishTable
OID | Name | Type | Access
.1 | Perm | ENUM | D
.2 | Service | ENUM | RW
.3 | Status | ENUM | RW
.4 | Interface | INTEGER | RW
.5 | User | DisplayString | RW
.6 | Password | DisplayString | RW
.7 | IPAddress | IpAddress | R
.8 | LastUpdate | Date | R
.9 | Retries | INTEGER | RW
.20 | DynProvider | INTEGER | RW
.21 | DynHostName | DisplayString | RW
.23 | DynWild | ENUM | RW
.24 | DynMX | DisplayString | RW
.25 | DynCheckDNS | DisplayString | RW
.26 | Description | DisplayString | RW
.27 | UseSSL | ENUM | RW
.28 | AuthEnforced | ENUM | RW
.29 | IpVersion | ENUM | RW
.30 | Ip6Address | InetAddressIPv6 | R
Perm
Controls the use of this dynamic DNS entry. Enumerations: enabled (1) disabled (2) delete (3)
Service
Uses LDAP or dynamic DNS protocol for IP Publishing. Enumerations: ldap (1) dyndns (2)
Status
The actual status of the publishing procedure. Enumerations: failed (1) update (2) updating (3) checking (4) up-to-date (5)
Interface
The interface corresponding to this entry.
User
The user identification for dynamic DNS ip address updates. Length: 0 to 255
Password
The password for the dynamic DNS service authentication. Length: 0 to 255
IPAddress
The IPv4 address which has been published last time. Relevant only if ipPublishIpVersion is set to 'ipv4'.
LastUpdate
The timestamp of the last update of either ipPublishIPAddress or ipPublishIp6Address. Range: 0 to -1
Retries
The # of retries if the update of the actual ip address fails.
DynProvider
The index of the dynamic DNS provider in the ipDynDnsProviderTable. Range: 0 to 10000
DynHostName
The hostname of the dynamic DNS service provider for ip address updates. Length: 0 to 255
DynWild
Enable or disable the use of Wildcards (provider specific). Enumerations: off (1) on (2)
DynMX
The mx info (provider specific). Length: 0 to 255
DynCheckDNS
The official DNS server of the provider to use for verification of the updated ip address (currently unused). Length: 0 to 255
Description
A textual string describing this dynDNS client entry. Length: 0 to 255
UseSSL
If enabled, the server URL will be changed to https(SSL). ipDdnsSupportsSSL must also be set to 'yes' in this case. Enumerations: yes (1) no (2)
AuthEnforced
If enabled, the server must authenticate itself to the CPE. ipPublishUseSSL must be set to 'yes' in this case. Enumerations: enabled (1) disabled (2)
IpVersion
The IP protocol family selector to be used for this entry. Enumerations: ipv4 (1) ipv6 (2)
Ip6Address
The IPv6 address which has been published last time. Relevant only if ipPublishIpVersion is set to 'ipv6'. Length: 16 to 16

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH