>> MIB - Management Information Base
>> Table: isdn - (.1.3.6.1.4.1.272.4.2)
isdn
OID | Name | Type | Access
.7 | AccountingTemplate | DisplayString | RW
.9 | LoginOnPPPDispatch | ENUM | RW
.10 | HistoryMaxEntries | INTEGER | RW
.13 | LoginSpeechMode | ENUM | RW
AccountingTemplate
Specifies the format of accounting messages sent by the syslog protocol. The format can consist of any order of the following variables. Tag Meaning %S Date the connection opened; in DD.MM.YY format. %s Time the connection was established: in HH:MM:SS format %R Date the connection closed; in DD.MM.YY format. %r Time the connection was closed: in HH:MM:SS format. %d The duration of the connection in seconds. %D Call identification: internal/external, ID, slot/unit (PABX only) %P Call classification: Private/Business, project number (PABX only) %y Total number of bytes received over the connection. %Y Total number of bytes sent over the connection. %g Total packets received over the connection %G Total packets sent over the connection. %c Total number of charging units (value) incurred for the connection. %C Total number of charging units (string) incurred for the connection. %n The call's direction; either incoming (I) or outgoing (O). %Z The local address (Calling or Called party's number, see %n). %z The local subaddress (Calling or Called party's number, see %n). %T The remote address (Calling or Called party's number %n). %t The remote subaddress (Calling or Called party's number %n). %i Service indicator and additional information for the call. %b Bearer capability for the call. %l Low layer capability for the call. %h High layer capability for the call. %u DSS1 error cause, if applicable. %U 1tr6 error cause, if applicable. %L Local (internal) error cause. %F Call reference (internal). %e Calling extension (for call assiciation; PABX only) %I Information about the subsystem the call was given to. The default accounting template setting contains the following tags: %S,%s,%r,%d,%y,%Y,%g,%G,%C,%n,%Z,%T,%i,%u,%L,%I. This template produces accounting messages similar to the following. ISDN:18.08.1997,13:53:19,13:53:34,12,1096,1875,33,33,1Units,O,2,091196730,7/0,9F,0 Length: 0 to 255
LoginOnPPPDispatch
Allows or disallows incoming ISDN calls (with an ISDN service indicator of 'telephony'), to be connected to the isdnlogin daemon even though the call has a matching service in the isdnDispatchTable (isdnDspItem). These calls must be initiated using isdnlogin <telno> telephony. Enumerations: allow (1) disallow (2)
HistoryMaxEntries
Maximum number of isdnCallHistory entries in memory. Range: 0 to 255
LoginSpeechMode
GFK request for modem dial in also if the requested service is not voice Enumerations: default (1) modem (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH