>> MIB - Management Information Base
>> Table: ipMRouteScopeNameTable - (.1.3.6.1.2.1.83.1.1.6.1)
Description: An entry (conceptual row) in the ipMRouteScopeNameTable representing a multicast scope name.
ipMRouteScopeNameTable
OID | Name | Type | Access
.1 | Address | IpAddress | R
.2 | AddressMask | IpAddress | R
.3 | Language | LanguageTag | R
.4 | String | SnmpAdminString | RC
.5 | Default | ENUM | RC
.6 | Status | ENUM | D
Address
The group address which when combined with the corresponding value of ipMRouteScopeNameAddressMask identifies the group range associated with the multicast scope. Scoped addresses must come from the range 239.x.x.x.
AddressMask
The group address mask which when combined with the corresponding value of ipMRouteScopeNameAddress identifies the group range associated with the multicast scope.
Language
The RFC 1766-style language tag associated with the scope name. Length: 1 to 100
String
The textual name associated with the multicast scope. The value of this object should be suitable for displaying to end-users, such as when allocating a multicast address in this scope. When no name is specified, the default value of this object should be the string 239.x.x.x/y with x and y replaced appropriately to describe the address and mask length associated with the scope. Length: 0 to 255
Default
If true, indicates a preference that the name in the following language should be used by applications if no name is available in a desired language. Enumerations: true (1) false (2)
Status
The status of this row, by which new entries may be created, or old entries deleted from this table. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH