>> MIB - Management Information Base
>> Table: mon4geSysConfigTable - (.1.3.6.1.4.1.272.4.41.5.1.1.1)
Description: A single mon4geSysConfigTable entry.
mon4geSysConfigTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Address | DisplayString | RW
.4 | Community | DisplayString | RW
.5 | Refresh | INTEGER | RW
Index
A unique index for this entry.
AdminStatus
Administration state. Enumerations: enable (1) disable (2) delete (3)
Address
Address of the 4Ge system to monitor. Format: FQDN or a valid IPv4 address. Length: 0 to 255
Community
The SNMP Read Community of the remote system. Length: 0 to 255
Refresh
The refresh Time in milliseconds. Range: 1000 to 60000

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH