>> MIB - Management Information Base
>> Table: tr069Persistent - (.1.3.6.1.4.1.272.4.22.6.2)
tr069Persistent
OID | Name | Type | Access
.1 | ProvisioningCode | DisplayString | RW
.7 | Bootstrap | ENUM | RW
.12 | FirstUseDate | Date | RW
.13 | ParameterKey | DisplayString | R
.14 | ACSServiceActiveUntil | Date | R
ProvisioningCode
Identifier of the primary service provider and other provisioning parameters. Length: 0 to 64
Bootstrap
Set on first startup or after ACS URL change to indicate bootstrap on next inform to the ACS. Enumerations: false (1) true (2)
FirstUseDate
This variable contains the first use date as specified for Device.DeviceInfo.FirstUseDate in TR-181 2.0[.1.] (first time synchronisation of device with a time server) NOTE: default value 0 means the 'Unknown Time' value. Range: 0 to -1
ParameterKey
This variable remembers TR-069 value ParameterKey as specified for Device.ManagementServer.ParameterKey in TR-069. Default value is the empty string. Length: 0 to 255
ACSServiceActiveUntil
This variable controls behavior of service LED in case an ACS can influence it by means of CWMP, i.e. by setting a TR-069 parameter. If variable value is in the future it specifies the time until which an indication by the service LED is to be kept active. Range: 0 to -1

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH