>> MIB - Management Information Base
>> Table: pppLqmTable - (.1.3.6.1.4.1.272.4.3.6.1)
Description: The pppLqmTable contains statistical information for each current PPP link on the system. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new PPP link was established and LQM negotiated successful. Deleting entries: Entries are removed by the system when the corresponding PPP link is disconnected.
pppLqmTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | CallReference | INTEGER | R
.3 | ReportingPeriod | INTEGER | R
.4 | OutLQRs | Counter | R
.5 | OutPackets | Counter | R
.6 | OutOctets | Counter | R
.7 | InLQRs | Counter | R
.8 | InPackets | Counter | R
.9 | InOctets | Counter | R
.10 | InDiscards | Counter | R
.11 | InErrors | Counter | R
.12 | PeerOutLQRs | Counter | R
.13 | PeerOutPackets | Counter | R
.14 | PeerOutOctets | Counter | R
.15 | PeerInLQRs | Counter | R
.16 | PeerInPackets | Counter | R
.17 | PeerInOctets | Counter | R
.18 | PeerInDiscards | Counter | R
.19 | PeerInErrors | Counter | R
.20 | LostOutLQRs | Counter | R
.21 | LostOutPackets | Counter | R
.22 | LostOutOctets | Counter | R
.23 | LostPeerOutLQRs | Counter | R
.24 | LostPeerOutPkts | Counter | R
.25 | LostPeerOutOcts | Counter | R
IfIndex
Correlating PPP interface index.
CallReference
The call reference of the dialup link, correlating to the isdnCallReference field in the isdnCallTable.
ReportingPeriod
The LQMReportingPeriod field indicates the maximum time in hundredths of seconds between transmission of Link Quality Reports (LQR). The peer may transmit packets at a faster rate than that which was negotiated.
OutLQRs
Number of transmitted Link Quality Reports (LQR) on this link.
OutPackets
Number of transmitted Packets on this link.
OutOctets
Number of transmitted Octets on this link, including framing data.
InLQRs
Number of Link Quality Reports (LQR) received on this link.
InPackets
Number of Packets reveived on this link.
InOctets
Number of Octets reveived on this link, including framing data.
InDiscards
Number of Packets received on this link, but discarded.
InErrors
Number of errorneous Packets received on this link.
PeerOutLQRs
Number of Link Quality Reports (LQR) transmitted by remote on this link.
PeerOutPackets
Number of Packets transmitted by remote on this link.
PeerOutOctets
Number of Octets transmitted by remote on this link, including framing data.
PeerInLQRs
Number of Link Quality Reports (LQR) received by remote on this link.
PeerInPackets
Number of Packets reveived by remote on this link.
PeerInOctets
Number of Octets reveived by remote on this link, including framing data.
PeerInDiscards
Number of Packets received by remote on this link, but discarded.
PeerInErrors
Number of errorneous Packets received by remote on this link.
LostOutLQRs
Number of lost Link Quality Reports (LQR) transmitted on this link.
LostOutPackets
Number of lost Packets transmitted on this link.
LostOutOctets
Number of lost Octets transmitted on this link.
LostPeerOutLQRs
Number of lost Link Quality Reports (LQR) transmitted by remote on this link.
LostPeerOutPkts
Number of lost Packets transmitted by remote on this link.
LostPeerOutOcts
Number of lost Octets transmitted by remote on this link.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH