>> MIB - Management Information Base
>> Table: mobilePdpContextTable - (.1.3.6.1.4.1.272.4.41.4.1.29.1)
Description: A single mobilePdpContextTable entry.
mobilePdpContextTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | IfIndex | INTEGER | R
.3 | PrimaryId | INTEGER | R
.4 | SecondaryId | INTEGER | R
.5 | Type | ENUM | R
.6 | APN | DisplayString | R
.7 | PreferredAddress | DisplayString | R
.8 | DataCompression | ENUM | R
.9 | HeaderCompression | ENUM | R
.10 | APNUser | DisplayString | R
.11 | APNPwd | DisplayString | R
Index
A unique index for this entry.
IfIndex
The interface index of the corresponding TTY interface.
PrimaryId
The primary PDP context identifier. Range: 1 to 16
SecondaryId
Shows the secondary PDP context identifier (non-zero). In case of a primary PDP context this object is zero. Range: 0 to 16
Type
The protocol type of the PDP context. This object is unused in case of a secondary PDP context. Enumerations: ipv4 (1) ppp (2) ipv6 (3) ipv4v6 (4)
APN
The APN (Access Point Name) used by the PDP context. This object is unused in case of a secondary PDP context. Length: 0 to 128
PreferredAddress
The preferred (IP-)Address assigned to the PDP context. Length: 0 to 64
DataCompression
The data compression used for data connections. This object is normally unused in 2G/3G/4G networks. Enumerations: off (1) on (2) v42bis (3) v44 (4)
HeaderCompression
The header compression used for data connections. This object is normally unused in 2G/3G/4G networks. Enumerations: off (1) on (2) rfc1144 (3) rfc2507 (4) rfc3095 (5)
APNUser
The APN (Access Point Name) Username used by the PDP context. Length: 0 to 80
APNPwd
The APN (Access Point Name) Password used by the PDP context. Length: 0 to 80

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH