>> MIB - Management Information Base
>> Table: biboAdmGuiAccessTable - (.1.3.6.1.4.1.272.254.14.1)
Description: The biboAdmGuiAccessTable defines 'required access level' for GUI access IDs.
biboAdmGuiAccessTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.3 | State | ENUM | D
.4 | RequiredLvlMask | HexValue | RW
Index
The GUI access index of the associated id.
State
Make entry valid/invalid or discard it. Enumerations: valid (1) delete (2) invalid (3)
RequiredLvlMask
Define required GUI access level bits. Available access levels bits reach from 0 to 30 Normal behavior: Only users get access to the part of GUI which is specified by biboAdmGuiAccessInedx, which have at least one bit set in biboAdmLoginGUIAccessMaks which is also set in here. System administrator and users which have admin rights (bit 1 (2)) in biboAdmLoginGUIAccessLevel have always access to any GUI part. This can be overruled by setting bit 0 in biboAdmGuiAccessRequiredLevel. Range: 0 to -1

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH