>> MIB - Management Information Base
>> Table: ip6DhcpSntpServerOptTable - (.1.3.6.1.4.1.272.4.5.100.4.8.1)
Description: Statically assigned SNTP-server-addresses (see 4 of RFC-4075). If multiple entries match then all related addresses are stored in a single SNTP-server-option according to sorting-order specified via 'ip6DhcpSntpServerOptListIdx'. If SNTP-option is requested but no entries match then DHCP-server returns own address if NTP-service of router is activated.
ip6DhcpSntpServerOptTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | ListIdx | INTEGER | RW
.6 | Address | InetAddressIPv6 | RW
Id
Internal identifier of this SNTP-entry.
AdminStatus
Activate/deactivate/delete this SNTP-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this SNTP-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this SNTP-entry is ignored. Range: 1 to 65535
ListIdx
Defines sorting-order in case of several matching SNTP-entries. Lower number means 'earlier in list'. Range: 0 to 255
Address
Address of SNTP-server. Length: 16 to 16

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH