>> MIB - Management Information Base
>> Table: mpsDoorIntercomSourceTable - (.1.3.6.1.4.1.272.4.53.7.2.1)
Description: This table contains the global information for each button of a door intercom.
mpsDoorIntercomSourceTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | Button | DoorButtonIndex | RW
.3 | SetupDTMF | DisplayString | RW
.4 | ForwardingTime | INTEGER | RW
.5 | ParallelTime | INTEGER | RW
.6 | AlertingTimeout | INTEGER | RW
.7 | Calendar | INTEGER | RW
.8 | AdminStatus | ENUM | D
.9 | Descr | DisplayString | RW
Index
A unique value for each door intercom. Reference to mpsDoorIntercomIndex. Range: 1 to 10
Button
A unique value for each button of a door intercom. Range: 1 to 4
SetupDTMF
A unique value for each door intercom and bell button. Length: 0 to 4
ForwardingTime
The linear and rotating doorline team calls allow you to configure a time interval in seconds, after which the next member of the doorline team will be called. Range: 1 to 99
ParallelTime
The linear and rotating doorline team calls allow you to configure a time interval in seconds, after which all members of the doorline team will be called at the same time. Range: 1 to 99
AlertingTimeout
The doorline team calls allow you to configure a time interval in seconds, how long the whole team will be called. Range: 0 to 99
Calendar
Select a calendar to switch the call mode automatically. After you have selected a calendar you can set the active call mode. 0 (not active), 1 (day mode), 2 (night mode).
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
Descr
Name of the button. Length: 0 to 32

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH