>> MIB - Management Information Base
>> Table: ipLoadBGroupTable - (.1.3.6.1.4.1.272.4.5.40.1)
Description: The ipLoadBGroupTable contains parameters related to the IP session-based load balancing algorithm. Each entry defines a load balancing interface group, the members of this group (interfaces) are associated via specific entries in the ipLoadBIfTable. Entries can only be added or deleted by the user. Creating entries: Entries are created by assigning a value to the ipLoadBGroupId object. Deleting entries: Entries are removed by setting an entry's ipLoadBGroupDistributionMode object to 'delete'.
ipLoadBGroupTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | Description | DisplayString | RW
.3 | DistributionPolicy | ENUM | RW
.4 | DistributionMode | ENUM | D
Id
Unique ID for the IP load balancing interface group. Range: 0 to 99
Description
Short Description for the IP load balancing interface group. Length: 0 to 255
DistributionPolicy
The distribution policy for the sesson-based IP load balancing algorithm. If set to round-robin(1) new IP sessions will be distributed to one member of the interface group according the ratio defined in ipLoadBIfTable (weighted round-robin policy). If set to load-dependent(2) new IP sessions will be distributed to one member of the group according the projected ratio (defined via ipLoadBIfTable) of bandwidth consumption in receive and transmit direction. If set to download-dependent(3) new IP sessions will be distributed to one member of the group according the projected ratio (defined via ipLoadBIfTable) of bandwidth consumption in receive direction (download only). If set to upload-dependent(4) new IP sessions will be distributed to one member of the group according the projected ratio (defined via ipLoadBIfTable) of bandwidth consumption in transmit direction (upload only). If set to static-routing(5) new sessions will be distributed according the source/destination IP addresses and/or protocols/services defined via specific ipExtRtTable entries. Enumerations: round-robin (1) load-dependent (2) download-dependent (3) upload-dependent (4) static-routing (5)
DistributionMode
The distribution mode for the sesson-based IP load balancing algorithm. This variable determines the ifOperStatus conditions of the IP load balancing interface group members to be considered for the session distribution procedure. If set to always(1) the interface is used either at once or - if the status is dormant - the ifAdminStatus is set to dialup to bring the interface in the up state. If set to up-only(2), the interfaces which are not in the up state will be ignored. Enumerations: always (1) up-only (2) delete (10)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH