>> MIB - Management Information Base
>> Table: voipSipLineTable - (.1.3.6.1.4.1.272.4.33.6.15.1)
Description: Describes an ISDN bundle definition entry.
voipSipLineTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Descr | DisplayString | RW
.3 | Mode | ENUM | D
.4 | Mask | BitValue | RW
Index
Unique index (interface index) of entry.
Descr
User defined description of line bundle. Length: 0 to 30
Mode
The mode of the bundle: 'external' -> bundle contains only TE PP ISDN ports; 'trunk' -> bundle contains only NT PP ISDN ports; 'delete' -> delete entry. Deafult value is external. Enumerations: external (1) trunk (2) delete (8)
Mask
Bitmask with those bits set to 1 for all ISDN interfaces used by this bundle entry. The corresponding ISDN interfaces can be found in isdnStkTable entries with 'isdnStkNumber' equal to bit position of set bits here. Range: 0 to -1

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH