>> MIB - Management Information Base
>> Table: wlcWlanIfProfileTable - (.1.3.6.1.4.1.272.4.61.1.17.1)
Description: This table contains WLAN interface profiles.
wlcWlanIfProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Name | DisplayString | RW
.3 | Type | ENUM | D
.4 | Mode | ENUM | RW
.5 | Speed | ENUM | RW
.6 | SkipChannels24GHz | BITS | RW
.7 | SkipChannels5GHz | BITS | RW
.8 | RtsThreshold | INTEGER | RW
.9 | FragmentationThreshold | INTEGER | RW
.10 | Burst | ENUM | RW
.11 | Country | DisplayString | RW
.12 | Band | ENUM | RW
.13 | AckWindow | INTEGER | RW
.14 | BeaconPeriod | INTEGER | RW
.15 | DTIMPeriod | INTEGER | RW
.16 | SpatialStreams | INTEGER | RW
.17 | Greenfield | ENUM | RW
.18 | ShortGI | ENUM | RW
.19 | RxSTBC | ENUM | RW
.20 | TxSTBC | ENUM | RW
.21 | FortyMHzOperation | ENUM | RW
.22 | ShortRetry | INTEGER | RW
.23 | LongRetry | INTEGER | RW
.24 | BgScanning | ENUM | RW
.25 | AirtimeFairness | ENUM | RW
.26 | Bandwidth | ENUM | RW
.27 | PresenceAnalytics | ENUM | RW
.28 | ACSOnBlocker | ENUM | RW
Index
Unique index of a WIFI interface profile.
Name
The name of the requested profile. Length: 0 to 255
Type
The WLAN physical interface type: off(1) interface disabled access-point(2) access point client(3) client mode delete(32) delete Enumerations: off (1) access-point (2) client (3) delete (32)
Mode
Mixed and compatibility modes between various 802.11 substandards. Enumerations: m802-11b (1) m802-11g (2) m802-11mixed (3) m802-11mixed-long (4) m802-11mixed-short (5) m802-11a (6) m802-11bgn (7) m802-11gn (8) m802-11n (10) m802-11an (11) m802-11abg (12) m802-11abgn (13) m802-11agn (14) m802-11anac (15) m802-11nac (16) m802-11ac (17) m802-11bgnax (18) m802-11gnax (19) m802-11nax (20) m802-11anacax (21) m802-11nacax (22) m802-11acax (23) m802-11ax (24)
Speed
The value defines the bitrate or the coding scheme to use for data frames. Default value auto(31) enables automatic rate adaption. Enumerations: s1mbit (1) s2mbit (2) s5mbit (3) s6mbit (4) s9mbit (5) s11mbit (6) s12mbit (7) s18mbit (8) s24mbit (9) s36mbit (10) s48mbit (11) s54mbit (12) sMCS0-HT (13) sMCS1-HT (14) sMCS2-HT (15) sMCS3-HT (16) sMCS4-HT (17) sMCS5-HT (18) sMCS6-HT (19) sMCS7-HT (20) sMCS8-HT (21) sMCS9-HT (22) sMCS10-HT (23) sMCS11-HT (24) sMCS12-HT (25) sMCS13-HT (26) sMCS14-HT (27) sMCS15-HT (28) auto (31) sMCS16-HT (32) sMCS17-HT (33) sMCS18-HT (34) sMCS19-HT (35) sMCS20-HT (36) sMCS21-HT (37) sMCS22-HT (38) sMCS23-HT (39)
SkipChannels24GHz
If a bit is set the according channel will be skipped from the channel scan list (channel 1-14 for 2.4 GHz). Default is to scan channels 1, 6 and 11. Enumerations: channel-1 (0) channel-2 (1) channel-3 (2) channel-4 (3) channel-5 (4) channel-6 (5) channel-7 (6) channel-8 (7) channel-9 (8) channel-10 (9) channel-11 (10) channel-12 (11) channel-13 (12) channel-14 (13)
SkipChannels5GHz
If a bit is set the accordingly channel will be skipped from the channel scan list (channel 36-173 for 5 GHz). Default is to scan all channels except 120, 124 and 128. Enumerations: channel-36 (0) channel-40 (1) channel-44 (2) channel-48 (3) channel-52 (4) channel-56 (5) channel-60 (6) channel-64 (7) channel-100 (8) channel-104 (9) channel-108 (10) channel-112 (11) channel-116 (12) channel-120 (13) channel-124 (14) channel-128 (15) channel-132 (16) channel-136 (17) channel-140 (18) channel-149 (19) channel-153 (20) channel-157 (21) channel-144 (22) channel-161 (23) channel-165 (24) channel-169 (25) channel-173 (26)
RtsThreshold
This attribute shall indicate the number of octets in an MPDU, below which an RTS/CTS handshake shall not be performed, except as RTS/CTS is used as a cross modulation protection mechanism. An RTS/CTS handshake shall be performed at the beginning of any frame exchange sequence where the MPDU is of type Data or Management, the MPDU has an individual address in the Address1 field, and the length of the MPDU is greater than this threshold. Setting this attribute to be larger than the maximum MSDU size shall have the effect of turning off the RTS/CTS handshake for frames of Data or Management type transmitted by this STA. Setting this attribute to one shall have the effect of turning on the RTS/CTS handshake for all frames of Data or Management type transmitted by this STA. The default value of this attribute shall be 2347. Range: 1 to 2347
FragmentationThreshold
This attribute shall specify the current maximum size, in octets, of the PSDU that may be delivered to the PHY. This maximum size does not apply in the case of A-MPDU. An MSDU, A-MSDU or MMPDU shall be broken into fragments if its size exceeds the value of this attribute after adding MAC headers and trailers. An MSDU, A-MSDU or MMPDU shall be fragmented when the resulting frame has an individual address in the Address1 field, and the length of the frame is larger than this threshold. The default value for this attribute shall be the lesser of 8000 or the aMPDUMaxLength or the aPSDUMaxLength of the attached PHY and shall never exceed the lesser of 8000 or the aMPDUMaxLength or the aPSDUMaxLength of the attached PHY. The value of this attribute shall never be less than 256. Default is 2346.
Burst
Sending wireless frames without backoff time. Enumerations: disabled (1) enabled (2)
Country
This attribute identifies the country in which the station is operating. The first two octets of this string are the two character country code as described in document ISO/IEC 3166-1. The third octet shall be one of the following: 1. an ASCII space character, if the regulations under which the station is operating encompass all environments in the country, 2. an ASCII 'O' character, if the regulations under which the station is operating are for an Outdoor environment only, or 3. an ASCII 'I' character, if the regulations under which the station is operating are for an Indoor environment only. Length: 0 to 3
Band
Frequency band. 'b24-GHz' -> 2.4 GHz band, 'b5-GHz' -> 5 GHz band, 'b58-GHz' -> 5.8 GHz band, 'b24-5-GHz' -> 2.4 GHz and 5 GHz band. Enumerations: b24-GHz (1) b5-GHz (2) b58-GHz (3) b24-5-GHz (4)
AckWindow
Additional 802.11 ACK timeout in microseconds. This must be set to non-zero value for radio distances larger than about 700m. Recommended setting is about 10 microseconds per kilometer.
BeaconPeriod
This attribute contains the number of TU that this BSS uses for scheduling Beacon transmissions.
DTIMPeriod
The number of DTIM intervals between the start of CFPs for this BSS.
SpatialStreams
This attribute indicates the maximum number of spatial streams enabled. The default value of this attribute is 4.
Greenfield
This attribute, when TRUE, indicates that the HT Greenfield option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortGI
This attribute, when TRUE, indicates that the Short Guard option is enabled for 40 MHz operation. The default value of this attribute is TRUE. Enumerations: true (1) false (2)
RxSTBC
This attribute, when TRUE, indicates that the entity's capability of receiving frames that are sent using the Space-Time Block Code (STBC) is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxSTBC
This attribute, when TRUE, indicates that the entity's capability of transmitting frames using Space-Time Block Code (STBC) option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
FortyMHzOperation
This attribute, when TRUE, indicates that the 40 MHz Operation is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortRetry
This attribute shall indicate the maximum number of transmission attempts of a frame, the length of which is less than or equal to dot11RTSThreshold, that shall be made before a failure condition is indicated. The default value of this attribute shall be 7.
LongRetry
This attribute shall indicate the maximum number of transmission attempts of a frame, the length of which is greater than dot11RTSThreshold, that shall be made before a failure condition is indicated. The default value of this attribute shall be 4.
BgScanning
Enable/disable background-scanning. Enumerations: disabled (1) enabled (2)
AirtimeFairness
If AirtimeFairness is enabled(1), background or best-effort traffic sent from AP to STA is fairly scheduled among all stations associated to this radio profile, in respect of airtime usage. The default value of this attribute is enabled(1). Enumerations: enabled (1) disabled (2)
Bandwidth
This attribute configures the maximum bandwidth. If this value is not equal to unused(1), this variable overwrite the value of wlcWlanIfProfileFortyMHzOperation. Enumerations: unused (1) b20MHz (2) b40MHz (3) b80MHz (4)
PresenceAnalytics
Enable/disable WLAN probe capturing on this interface. Enumerations: enabled (1) disabled (2)
ACSOnBlocker
When enabled(1), the radio module will switch to a new channel on presence of a blocking signal. Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH