>> MIB - Management Information Base
>> Table: ip6MldListenTable - (.1.3.6.1.4.1.272.4.5.100.2.8.1)
Description: A Mld 'Listen Entry' used by multicast routing.
ip6MldListenTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | Group | InetAddressIPv6 | R
.3 | Age | TimeStamp | R
.4 | Proto | BITS | R
IfIndex
Indicates the interface associoted with this Mld 'Listen Entry'. Range: 1 to 2147483647
Group
The listeners 'Multicast Group Address'. Length: 16 to 16
Age
Shows the age of the last active 'Listen Report' inititated by a client.
Proto
The listeners 'Protocol'. Enumerations: local (0) mld (1)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH