>> MIB - Management Information Base
>> Table: systemPhoneFunctionKeyTable - (.1.3.6.1.4.1.272.4.64.2.2.1)
Description: This table contains information concerning system phone function key configuration.
systemPhoneFunctionKeyTable
OID | Name | Type | Access
.1 | Index | SystelFunctionKeyIndex | RW
.2 | ModuleIndex | SystelModuleIndex | RW
.3 | Button | SystelFKButtonIndex | RW
.4 | Level | SystelFKLevel | RW
.5 | Description | DisplayString | RW
.6 | Type | ENUM | RW
.7 | MSNPrio | INTEGER | RW
.8 | TargetIndex | SystelTargetIndex | RW
.9 | TargetString | DisplayString | RW
.10 | AdminStatus | ENUM | D
Index
A unique value for each function key of a system phone. Range: 1 to 65535
ModuleIndex
Variable contains the index of the systemPhoneModuleTable as reference. Range: 1 to 65535
Button
Identifier for each function key. Valid range for systemPhoneFKButton for T400 is 1..22. Valid range for systemPhoneFKButton for T500 is 1..30. Range: 1 to 38
Level
Identifier for the (shift) level of each function key. One short press activates level 0 function, double press activates level 1 function. Range: 0 to 1
Description
The variable contains a short description of the key type, which may be printed on the system telephone label. Length: 0 to 20
Type
Specifies type of function key: dial-standard: standard speed dialing key. dial-dtmf: dials a DTMF sequence. dial-keypad: dials a keypad sequence. extension-subscriber: line key with LED and pickup function for user extension. extension-team: line key with LED and pickup function for team extension. trunk-line: trunk line key to establish next call via a configured trunk line. team-log: log an extension in or out of a team. system-call-announce: announcement to a choosen extension. system-call-announce-allow: allow/restrict incoming announcement inquiries. system-call-exchange: build up a call exchange connection between system phone and choosen extension. system-call-exchange-allow: allow/restrict incoming call exchange inquiries. boss-boss: key has to configure on boss system phone to call the secretary (special line key). boss-secretary: key has to configure on secretary system phone to call the boss (special line key). boss-diversion: key has to configure on boss system phone to divert incoming calls to secretary's phone. call-forwarding-cfu: activate/deactivate call forwarding immediately for an associated extension to a choosen internal number. call-forwarding-cfb: activate/deactivate call forwarding on busy for an associated extension to a choosen internal number. call-forwarding-cfnr: activate/deactivate call forwarding if no reply for an associated extension to a choosen internal number. macro: macro key (configuration only via system phone). headset: prepare a headset call (off-hook) or accept an incoming call with the headset. auto-accept: activate/deactivate automatic call accpetance. bundle: establish next call via a configured bundle (trunk group). connection: key to change between two calls (for the correct function of this function key type you have to configure at least 2 connection keys, to switch between the connections). system-parking: depositing a subscriber to configured system parking place (open inquiry) or fetch a subscriber from system parking place. internal-line-access: get internal call waiting tone if automatic outside line access is activated. hotel-room: key has to configure on first level of reception system phone to checkin or checkout hotel rooms. agent-time: key has to configure on first level of agent system phone to activate/deactivate agent time for associated agent. night-mode: activate/deactivate the PBX nightmode (eg. for switching variants of teams, TFE, CoS, etc.). hotel-room-connect: key is automatically set to second level on system phone if a hotel-room is configured, with a double press the reception can establish a call to choosen hotel room. agent-time-renew: key is automatically set to second level on system phone if a agent-time is configured, with a double press the agent can renew the associated agent timer. do-not-disturb: activate / deactivate the do not disturb mode of NG system phones (settings for this mode have to be modified in systemPhoneFacilityTable). shift: this key has to be configured as alternative to the double keypress to get access to the second level function keys. parallel-ringing: this key activates or deactivates the parallel ringing option. nop: this key is only a dummy key and leads to no operation in system phone. It is usefull to use this keytype if second level should be locked. system-call-announce-team: announcement to a team. msn-selection: use a specific MSN for outgoing call (CLIP signalling). xml-content: gigaset-> XML Mini Browser (URL). next-call-anonymous: gigaset-> set CLIR for next call. menu-call-divert: gigaset-> menu call diversion. menu-resource-dir: gigaset-> menu media pool. menu-internet-radio: gigaset-> menu internet radio. toggle-call-divert: gigaset-> call diversion on/off. not-configured: gigaset-> This function key is not configured and therefore will not be set via provisioning. (That means: Do not touch! This key is controlled by the device itself.) Enumerations: dial-standard (1) dial-dtmf (2) dial-keypad (3) extension-subscriber (4) extension-team (5) trunk-line (6) team-log (7) system-call-announce (8) system-call-announce-allow (9) system-call-exchange (10) system-call-exchange-allow (11) boss-boss (12) boss-secretary (13) boss-diversion (14) call-forwarding-cfu (15) call-forwarding-cfb (16) call-forwarding-cfnr (17) macro (18) headset (19) auto-accept (20) bundle (21) connection (22) system-parking (23) internal-line-access (24) hotel-room (25) agent-time (26) night-mode (27) hotel-room-connect (28) agent-time-renew (29) do-not-disturb (30) shift (31) parallel-ringing (32) nop (33) system-call-announce-team (34) msn-selection (35) xml-content (50) next-call-anonymous (51) menu-call-divert (52) menu-resource-dir (53) menu-internet-radio (54) toggle-call-divert (55) not-configured (99)
MSNPrio
This variable contains the index of the selected MSN within the phone, for which this function shall be activated. Only used when selecting the systemPhoneFKType: team-log, call- forwarding-xxx or auto-accept. 1 .. 12: The function key is attributed to a specific MSN. 0: The function key is attributed to the default MSN. Range: 0 to 12
TargetIndex
The variable contains either ExtensionIndex, GroupIndex, TrunkGroupIndex, TrunkBundleIndex or SystemNumberPosition, depending upon the function key type selected. Range: 1 to 65535
TargetString
Variable contents depends upon the function key configured. It may be either a dialling number, a DTMF sequence, a keypad sequence, a call forwarding target number or a macro key sequence. Length: 0 to 255
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH