>> MIB - Management Information Base
>> Table: bacAddressTable - (.1.3.6.1.4.1.272.4.60.1.5.1)
Description: One entry in bacAddressTable.
bacAddressTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | PropertyIndex | INTEGER | RW
.3 | IpAddress | IpAddress | RW
.4 | IpNetmask | IpAddress | RW
.5 | Domain | DisplayString | RW
.6 | AdminStatus | ENUM | D
.7 | InetAddressType | ENUM | RW
.8 | InetAddress | InetAddress | RW
.9 | InetAddressPrefixLength | InetAddressPrefixLength | RW
Index
The index in this IP address table. Range: 1 to 65535
PropertyIndex
Index of entry in bacPropertyTable to be referenced. Range: 1 to 65535
IpAddress
The address defining the IP address range.
IpNetmask
The netmask defining the IP address range.
Domain
The domain name defining the address. If empty bacAddressIpAddress and bacAddressIpNetmask is used. Length: 0 to 255
AdminStatus
If the AdminStatus is set to enabled(1) this entry will be used, if set to disabled(2) it won't be used. You may also delete this entry by changing it to delete(3). Enumerations: enabled (1) disabled (2) delete (3)
InetAddressType
Fields (AddressType, Address, PrefixLength) specify address or subnet of the following address type: ipv4 -- IPv4 address, allowed PrefixLength range is [0..32]. ipv6 -- IPv6 address, allowed PrefixLength range is [0..128]. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
InetAddress
See description of AddressType field. Length: 0 to 255
InetAddressPrefixLength
See description of AddressType field. Range: 0 to 2040

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH