>> MIB - Management Information Base
>> Table: mobileAdmOperatorTable - (.1.3.6.1.4.1.272.4.41.4.1.30.1)
Description: A single mobileAdmOperatorTable entry.
mobileAdmOperatorTable
OID | Name | Type | Access
.1 | IccId | DisplayString | RW
.2 | Code | Unsigned32 | RW
.3 | Name | DisplayString | RW
.4 | AcT | BITS | RW
.5 | Priority | INTEGER | RW
.6 | Status | ENUM | D
IccId
The ICC-ID of the SIM-Card. The operator is assigned to this SIM Id. Length: 0 to 20
Code
The PLMN Code is built from a 3 digit MCC (Mobile Country Code) and 2 or 3 digit MNC (Mobile Network Code).
Name
The name of the network operator. Length: 0 to 40
AcT
The AcT defines the Access technologies gsm - G2 connectivity umts - G3 connectivity lte - G4 connectivity Enumerations: gsm (1) umts (2) lte (3)
Priority
This value represents the relative priority of this entry. it is added to the admistrative base priority (see 'mobileOperatorPriority') to be used afterwards for the operator selection procedure. Under normal circumstances it's intended that this resulting priority is higher than the priority values associated with the priviledged and preferred operators read from SIM card.
Status
The operator's status. permit - the operator is allowed for roaming. deny - the operator is forbidden to use. delete - delete this entry Enumerations: permit (1) deny (2) delete (8)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH