>> MIB - Management Information Base
>> Table: ip6DhcpDomainNameOptTable - (.1.3.6.1.4.1.272.4.5.100.4.10.1)
Description: Statically assigned domain-search-names (see 4 of RFC-3646). If multiple entries match then all related domain-names are stored in a single domain-list-option according to sorting-order specified via 'ip6DhcpDomainNameOptListIdx'.
ip6DhcpDomainNameOptTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | ListIdx | INTEGER | RW
.6 | Value | DisplayString | RW
.7 | FullValue | DisplayString | R
Id
Internal identifier of this domain-entry.
AdminStatus
Activate/deactivate/delete this domain-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this domain-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this domain-entry is ignored. Range: 1 to 65535
ListIdx
Defines sorting-order in case of several matching domain-names. Lower number means 'earlier in list'. Range: 0 to 255
Value
Fully qualified domain-name to be added to search-list. Fully qualified domain-names must have trailing dot for distinction from relative/partial domain-names. However, many users/admins tend to forget this. Thus, 'proper version' of this field is stored in field 'FullValue'. Length: 0 to 255
FullValue
'Proper' fully qualified domain-name. See description of field 'Value'. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH