>> MIB - Management Information Base
>> Table: mpsReRouteApplModeTable - (.1.3.6.1.4.1.272.4.53.13.6.1)
Description: This table contains reroute information for each rerouting application and mode.
mpsReRouteApplModeTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | ApplIndex | ReRouteApplIndex | RW
.3 | ModeNumber | Unsigned32 | RW
.4 | RerouteIndex | ReRouteIndexOrZero | RW
.5 | AdminStatus | ENUM | D
Index
A unique value for each entry.
ApplIndex
This variable contains the reroute application index. Reference to mpsReReouteApplTable. Range: 1 to 65535
ModeNumber
For each rerouting application index, several modes can exist.
RerouteIndex
Index of the ReRouting function in mpsReRouteTable. Value 0 means that ReRouting function is inactive. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH