>> MIB - Management Information Base
>> Table: wlanVSSAuthTable - (.1.3.6.1.4.1.272.4.46.27.1)
Description: The wlanVSSAuth does contain some authentication parameters for a VSS.
wlanVSSAuthTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | ReAuthPeriod | INTEGER | RW
.3 | GroupRekeyStrict | ENUM | RW
.4 | GroupRekeyTime | INTEGER | RW
.5 | BlacklistTrials | INTEGER | RW
.6 | BlacklistTime | INTEGER | RW
.7 | BlacklistDuration | Unsigned32 | RW
IfIndex
Reference to VSS entry (wlanVSSIfIndex) this authentication parameters correspond to.
ReAuthPeriod
EAP reauthentication period in seconds (0=disabled).
GroupRekeyStrict
Rekey GTK when any STA that possesses the current GTK is leaving the BSS.
GroupRekeyTime
Time interval for rekeying GTK (broadcast/multicast encryption keys) in seconds.
BlacklistTrials
The number of failed authentication trails per wlanVSSAuthBlacklistTime before a station is stored into the dynamic blacklist.
BlacklistTime
The time within a station may perform wlanVSSAuthBlacklistTrials failed authentication trials, before it is temporarily blacklisted.
BlacklistDuration
The time a station is kept in the dynamic blacklist after too many failed authentication attempts. A value of 0 indicates that deletion is handled by a WLan Controller not the WLan driver.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH