>> MIB - Management Information Base
>> Table: ipBootpRelayTable - (.1.3.6.1.4.1.272.4.5.55.1.1)
Description: Interfaces that are enabled for BOOTP relay mode.
ipBootpRelayTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Enabled | ENUM | D
.3 | Server1 | IpAddress | RW
.4 | Server2 | IpAddress | RW
.5 | DiscoverOptionsGroupID | INTEGER | RW
.6 | RequestOptionsGroupID | INTEGER | RW
.7 | InformOptionsGroupID | INTEGER | RW
.8 | OfferOptionsGroupID | INTEGER | RW
.9 | AckOptionsGroupID | INTEGER | RW
.10 | DnsAssign | ENUM | RW
.11 | OutboundInterface1 | INTEGER | RW
.12 | OutboundInterface2 | INTEGER | RW
.13 | OutboundPort | ENUM | RW
IfIndex
Index of interface which will use BOOTP relay.
Enabled
Enable, disable or delete the table entry. Enumerations: delete (1) true (2) false (3)
Server1
The IP address of the first BOOTP server to use.
Server2
The IP address of the second BOOTP server to use.
DiscoverOptionsGroupID
Identifies the option or set of options which are added to the original DHCP DISCOVER message received from the client before forwarding it to the DHCP server. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. Range: 0 to 65535
RequestOptionsGroupID
Identifies the option or set of options which are added to the original DHCP REQUEST message received from the client before forwarding it to the DHCP server. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. Range: 0 to 65535
InformOptionsGroupID
Identifies the option or set of options which are added to the original DHCP INFORM message received from the client before forwarding it to the DHCP server. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. Range: 0 to 65535
OfferOptionsGroupID
Identifies the option or set of options which are added to the original DHCP OFFER message received from the DHCP server before forwarding it to the DHCP client. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. Range: 0 to 65535
AckOptionsGroupID
Identifies the option or set of options which are added to the original DHCP ACK message received from the DHCP server before forwarding it to the DHCP client. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. Range: 0 to 65535
DnsAssign
This variable determines the assignment policy, if set to passthrough (1) the DHCP domain server tag(s) will be passed unchanged, if set to self (2) the own IP address is provided as first nameserver address. Enumerations: passthrough (1) self (2)
OutboundInterface1
Optional index of the outbound interface to be used in conjunction with ipBootpRelayServer1. If not set (default) this interface is selected automatically due to the current status of the IP routing data base.
OutboundInterface2
Optional index of the outbound interface to be used in conjunction with ipBootpRelayServer2. If not set (default) this interface is selected automatically due to the current status of the IP routing data base.
OutboundPort
Determines the UDP source port to be used for the DHCP relay functionality. If set to bootpc(1), the common source port 68 (BOOTP client) will be used. If set to bootps(2) source port 67 (BOOTP server) will be used instead. Enumerations: bootpc (1) bootps (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH