>> MIB - Management Information Base
>> Table: capiConfigTable - (.1.3.6.1.4.1.272.4.7.6.1)
Description: The capiConfigTable contains configuration information for each ISDN stack. Setting these fields is optional, and is not required. Creating entries: Entries are created automatically by the system when a new ISDN stack is initialised in the isdnStkTable. Deleting entries: An entry can be removed by assigning the value `delete' to its capiConfigFaxG3RcvSpeed object. It can be removed only if there is no entry with it's capiConfigStkNumber in the isdnStkTable.
capiConfigTable
OID | Name | Type | Access
.1 | StkNumber | INTEGER | R
.2 | FaxG3RcvSpeed | ENUM | D
.3 | FaxG3ECM | ENUM | RW
.4 | FaxG3Header | ENUM | RW
.5 | VoiceCoding | ENUM | RW
.6 | SendAlerting | ENUM | RW
.7 | V42bis | ENUM | RW
.8 | ModemDefault | ENUM | RW
.9 | FaxModulation | ENUM | RW
.10 | Fax12000 | ENUM | RW
.11 | FaxTXLevel | ENUM | RW
StkNumber
The isdnStkNumber this configuration belongs to. Range: 0 to 31
FaxG3RcvSpeed
The G3 facsimile receive speed. For CM-EBRI this should be set to maximum. Set this field to `delete' to remove this entry. The entry can be deleted only if there is no entry with it's capiConfigStkNumber in the isdnStkTable. Enumerations: r4800 (1) r7200 (2) r9600 (3) r14400 (4) maximum (5) not-available (6) delete (7)
FaxG3ECM
Specifies whether ECM (error correction mode) should be used for G3 facsimile transmissions. Enumerations: on (1) off (2) not-available (3)
FaxG3Header
Specifies whether the header-line and logo ('BIANCA/FAX'), should appear on outgoing facsimiles. The value 'logo_header' allows the header-line and the logo to be printed on the top of each page. Enumerations: logo-header (1) no-logo (2) no-header (3) not-available (4)
VoiceCoding
Switches the bit order for voice-data. Enumerations: normal (1) reverse (2)
SendAlerting
For CAPI 1.1 this specifies when the CAPI server should send alert messages for incoming calls. Enumerations: never (1) ever (2) voice-only (3)
V42bis
Specifies whether V.42bis data compression should be used. If data compression is activated here,the receiving or sending side is first queried whether it supports data compression. The BRICK supports V.42bis data compression using up to 2 B-channels. Enumerations: on (1) off (2) not-available (3)
ModemDefault
Specifies the modem profile of the mdmProfileTable which contains the default modem parameters to use for modem connections. Enumerations: modem-profile-1 (1) modem-profile-2 (2) modem-profile-3 (3) modem-profile-4 (4) modem-profile-5 (5) modem-profile-6 (6) modem-profile-7 (7) modem-profile-8 (8)
FaxModulation
Set the default transmission protocol for fax. - v17 max. 14400 Bps new standard - v33 max. 14000 Bps early standard - v29 max. 9600 Bps fax standard - v17s v17 with Swiss capability - v33s v33 with Swiss capability Enumerations: v17 (1) v33 (2) v29 (3) v17s (5) v33s (6)
Fax12000
Enable or disable the 12000Bps Mode for fax transmission. A lot of fax receivers have problems with this tranmission mode. Default value is off Enumerations: on (1) off (2)
FaxTXLevel
Set the transmit level to -x dB db0 = 0dB, db3 = -3dB. In Germany -6dB (db6) is normally used for facsimile transmission. Enumerations: db0 (1) db3 (2) db6 (3) db9 (4) db12 (5) db15 (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH