>> MIB - Management Information Base
>> Table: wlcStaticBlacklistProfileTable - (.1.3.6.1.4.1.272.4.61.1.32.1)
Description: The wlcStaticBlacklistProfile contains information about stations that are blacklisted due to administrative actions.
wlcStaticBlacklistProfileTable
OID | Name | Type | Access
.1 | STAMac | MacAddress | RC
.2 | VSSProfIndex | INTEGER | RC
.3 | RowStatus | ENUM | D
STAMac
The MAC address of the station to blacklist. Length: 6 to 6
VSSProfIndex
The SSID (wlcVSSProfileIndex) this blacklist entry is associated to.
RowStatus
The row-status of a blacklist entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH