>> MIB - Management Information Base
>> Table: isdnDChanX31Table - (.1.3.6.1.4.1.272.4.2.6.1)
Description: The isdnDChanX31Table contains information for the X.31 stack for each available ISDN D-channel. This information is mainly used for X.25 packet-switching functions but can be used for CAPI applications. The table is initialized during the auto configure process. By default the system polls each D-channel for an assigned TEI (terminal endpoint identifier). Creating entries: Entries can be added by assigning a new value (valid IfIndex) to isdnX31IsdnIfIndex. Deleting entries: Entries are removed by assigning 'delete' to the approprate isdnX31IsdnAssignedTo object.
isdnDChanX31Table
OID | Name | Type | Access
.1 | IsdnIfIndex | INTEGER | RW
.2 | TeiProc | ENUM | RW
.3 | TeiValue | INTEGER | RW
.5 | AssignedTo | ENUM | D
.6 | IsdnPTIfIndex | INTEGER | RW
IsdnIfIndex
The corresponding ISDN interface that is used for this call. Refer to the isdnIfTable.
TeiProc
The procedure used for polling of TEI (terminal end-point identifiers) values. Enumerations: auto (1) fixed (2)
TeiValue
The TEI value for this interface. Range: -1 to 126
AssignedTo
The service this TEI value is assigned to. Enumerations: packet-switch (1) capi-default (2) capi (3) delete (4) pass-through (5)
IsdnPTIfIndex
The corresponding ISDN interface that is used as destination for this call in case variable isdnX31AssignedTo contains value pass-through. Refer to isdnIfTable.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH