>> MIB - Management Information Base
>> Table: mpsExtensionTable - (.1.3.6.1.4.1.272.4.53.6.1.1)
Description: This table contains all internal extensions.
mpsExtensionTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | IfIndex | InterfaceIndexOrZero | RW
.3 | DeviceVirtualIndex | INTEGER | RW
.4 | Number | DisplayString | RW
.5 | DisplayName | DisplayString | RW
.6 | AuthName | DisplayString | RW
.7 | AdminStatus | ENUM | D
.8 | User | UserIndexOrZero | RW
.9 | FacStatus | ENUM | R
.10 | Facilities | BITS | RW
.11 | ChargeCounter | INTEGER | RW
.12 | ReRouteAppl | ReRouteApplIndexOrZero | RW
Index
A unique value for each internal extension. Range: 1 to 65535
IfIndex
InterfaceIndex where the extension is placed. Range: 0 to 2147483647
DeviceVirtualIndex
This variable contains the virtual device index of the mpsDeviceVirtual table, if the mpsExtensionIfIndex is zero.
Number
This variable contains the internal number for the extension. Length: 0 to 4
DisplayName
Internal name of the extension. This name will be displayed as internal calling party. Length: 0 to 20
AuthName
Login name for VoIP-registration at the PBX. Length: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
User
This variable contains the reference to mpsUserIndex in mpsUserTable. Range: 0 to 65535
FacStatus
This variable contains the status for this extension. This status is set from call control to handle ccbs or ccnr (barred), room-supervision or temporarily trunk access for this extension. Enumerations: idle (1) barred (2) room-supervision (3) trunk-transfered (4)
Facilities
Extension facilities. mwi-tone : message waiting indication -> special tone. Enumerations: mwi-tone (0)
ChargeCounter
This variable contains current total charge counter for this extension. This value is standardized to a thousandth. Update via acctStoreTable. Cleanup this charge counter, set to '-1'.
ReRouteAppl
Index of ReRouting application in mpsReRouteApplTable. Value 0 means that ReRouting application is inactive. Range: 0 to 65535

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH