>> MIB - Management Information Base
>> Table: mpsHotelConfig - (.1.3.6.1.4.1.272.4.53.16.1)
mpsHotelConfig
OID | Name | Type | Access
.1 | Active | ENUM | RW
.2 | Reception1 | ExtensionIndexOrZero | RW
.3 | Reception2 | ExtensionIndexOrZero | RW
.4 | WakeUpChoice | BITS | RW
.5 | ChargeMultiplier | INTEGER | RW
.6 | ChargeExponent | INTEGER | RW
.7 | PrintHeader | DisplayString | RW
.8 | PrintFooter | DisplayString | RW
.9 | Facilities | BITS | RW
Active
This value determines, if system hotel functions are active or not. Enumerations: true (1) false (2)
Reception1
This variable contains the first reception phone. Reference to mpsExtensionTable. Range: 0 to 65535
Reception2
This variable contains the second reception phone. Reference to mpsExtensionTable. Range: 0 to 65535
WakeUpChoice
If the bit is set, the wakeUp announcement at check-in is selectable via menue access. Enumerations: reception1 (0) reception2 (1)
ChargeMultiplier
Charge rate multiplier. e.g. 1 Unit = 0,064 -> mpsHotelConfigChargeMultiplier = 64, mpsHotelConfigChargeExponent = -3. 1 Unit = 1,200 -> mpsHotelConfigChargeMultiplier = 12, mpsHotelConfigChargeExponent = -1
ChargeExponent
Charge rate exponent. e.g. 1 Unit = 0,064 -> mpsHotelConfigChargeMultiplier = 64, mpsHotelConfigChargeExponent = -3. 1 Unit = 1,200 -> mpsHotelConfigChargeMultiplier = 12, mpsHotelConfigChargeExponent = -1
PrintHeader
Definition of header for charging bill printout (at reception) at checkout. Length: 0 to 255
PrintFooter
Definition of footer for charging bill printout (at reception) at checkout. Length: 0 to 255
Facilities
Hotel global facilities: room-to-room-call-barring : room to room calls are not allowed. Enumerations: room-to-room-call-barring (0)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH