>> MIB - Management Information Base
>> Table: wlcRadiusSrvProfileTable - (.1.3.6.1.4.1.272.4.61.1.7.1)
Description: The wlcRadiusSrvProfileTable describes different RADIUS service profiles.
wlcRadiusSrvProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AddressType | ENUM | RW
.3 | Address | IpAddress | RW
.4 | Port | INTEGER | RW
.5 | Secret | DisplayString | RW
.6 | Priority | INTEGER | RW
.7 | Timeout | INTEGER | RW
.8 | Retries | INTEGER | RW
.9 | State | ENUM | D
.10 | KeepAlive | ENUM | RW
.11 | Protocol | ENUM | RW
Index
Unique index of a RADIUS service profile.
AddressType
The IP address type of the requested RADIUS service can be: -unknown(0): an unknown address type -ipv4(1) : an IPv4 address -ipv6(2) : an IPv6 address -ipv4z(3) : a non-global IPv4 address including a zone index -ipv6z(4) : a non-global IPv6 address including a zone index -dns(16) : a DNS domain name Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Address
The RADIUS Server IP Address.
Port
The RADIUS server authentication port. Please notice that RFC2138 assigns ports 1812 and 1813 for authentication and accounting, respectively. Many RADIUS servers still use the formerly assigned ports 1645 and 1646 instead. The default value is 1812. Range: 0 to 65535
Secret
The shared secret between RADIUS server and Brick. Length: 0 to 63
Priority
The RADIUS server with the lowest priority is the first used for request. If there is no response (see also the values Timeout and Retries) the RADIUS server with the next lowest priority will be used.
Timeout
The amount of milliseconds (1/1000s) waiting for an outstanding request.
Retries
The number of retries sent for each request, until the server state is set to inactive. Default value is 1. To prevent the radiusSrvState ever switch to inactive, set this value to 0.
State
When operational, the server state is active(1). If the RADIUS server does not respond, its state is set to inactive(2). The administrator can set the state manually to disabled(3), or delete(32) the entry. Enumerations: active (1) inactive (2) disabled (3) delete (32)
KeepAlive
Enables the periodicaly keep alive check of 'inactive' (see radiusSrvState) server. Enumerations: true (1) false (2)
Protocol
Type of authentication server. Allowed values are a subset of those specified for field radiusSrvProtocol (-> file mibradius). Enumerations: accounting (2) wpa802-1x (5)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH