>> MIB - Management Information Base
>> Table: tcpConnTable - (.1.3.6.1.2.1.6.13.1)
Description: A conceptual row of the tcpConnTable containing information about a particular current TCP connection. Each row of this table is transient, in that it ceases to exist when (or soon after) the connection makes the transition to the CLOSED state.
tcpConnTable
OID | Name | Type | Access
.1 | State | ENUM | D
.2 | LocalAddress | IpAddress | R
.3 | LocalPort | INTEGER | R
.4 | RemAddress | IpAddress | R
.5 | RemPort | INTEGER | R
.6 | IfIndex | INTEGER | R
State
The state of this TCP connection. The only value which may be set by a management station is deleteTCB(12). Accordingly, it is appropriate for an agent to return a `badValue' response if a management station attempts to set this object to any other value. If a management station sets this object to the value deleteTCB(12), then this has the effect of deleting the TCB (as defined in RFC 793) of the corresponding connection on the managed node, resulting in immediate termination of the connection. As an implementation-specific option, a RST segment may be sent from the managed node to the other TCP endpoint (note however that RST segments are not sent reliably). Enumerations: closed (1) listen (2) synSent (3) synReceived (4) established (5) finWait1 (6) finWait2 (7) closeWait (8) lastAck (9) closing (10) timeWait (11) deleteTCB (12)
LocalAddress
The local IP address for this TCP connection. In the case of a connection in the listen state which is willing to accept connections for any IP interface associated with the node, the value 0.0.0.0 is used.
LocalPort
The local port number for this TCP connection. Range: 0 to 65535
RemAddress
The remote IP address for this TCP connection.
RemPort
The remote port number for this TCP connection. Range: 0 to 65535
IfIndex
The interface over which the TCP connection is routed initial.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH