>> MIB - Management Information Base
>> Table: voipSpecialNumberTable - (.1.3.6.1.4.1.272.4.33.25.1)
Description: Describes a special number rule
voipSpecialNumberTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Descr | DisplayString | RW
.4 | Number | DisplayString | RW
.5 | Interface | INTEGER | RW
.6 | Convert | DisplayString | RW
Index
The unique Index value for this entry. Range: 1 to 65535
AdminStatus
The administrative state of this entry. Enumerations: enabled (1) disabled (2) delete (3)
Descr
Description of this entry. Length: 0 to 255
Number
The Special Number for handling. Length: 0 to 255
Interface
(Used in MGW mode only!) Optional: The fixed outgoing VoIP Interface for this special address, independent from any other call routing. Default: If this value is 0, the standard call routing is used to retrieve the outgoing interface but any conversion rules specified in the call routing entry are skipped and only the numbers defined in this entry are dialed instead.
Convert
Optional: The new special number if the outgoing interface uses a different number format. Default: Empty. No conversion is done. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH