>> MIB - Management Information Base
>> Table: ikeProfileTable - (.1.3.6.1.4.1.272.4.26.14.1)
Description: This object contains an IPSec phase 1 profile.
ikeProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Description | DisplayString | RW
.3 | AuthMethod | ENUM | D
.4 | Mode | ENUM | RW
.5 | Proposal | INTEGER | RW
.6 | Group | INTEGER | RW
.7 | Cert | INTEGER | RW
.8 | LocalId | DisplayString | RW
.9 | CaCerts | DisplayString | RW
.10 | LifeTime | INTEGER | R
.11 | PfsIdentity | ENUM | RW
.12 | Heartbeats | ENUM | RW
.13 | BlockTime | INTEGER | RW
.14 | NatT | ENUM | RW
.15 | MtuMax | INTEGER | RW
.16 | LifeSeconds | Unsigned32 | RW
.17 | LifeKBytes | Unsigned32 | RW
.18 | LifeRekeyPercent | INTEGER | RW
.19 | LifePolicy | ENUM | RW
.20 | Ip6MtuMax | INTEGER | RW
Index
A unique index identifying this entry.
Description
An optional description for this profile.
AuthMethod
This object specifies the authentication method used for this profile. Possible values: pre-sh-key(1), -- Authentication using pre shared keys dss-sig(2), -- Authentication using DSS signatures rsa-sig(3), -- Authentication using RSA signatures rsa-enc(4), -- Authentication using RSA encryption default(14), -- use settings from default profile -- (pre-sh-key if this is the default profile) delete(15) -- mark this entry for deletion.
Mode
This object specifies the exchange mode used for IKE SA negotiation. Possible values: id-protect(1), -- Use identity protection (main) mode aggressive(2), -- Use aggressive mode default(3), -- Use default setting from the -- global profile id-protect-only(4), -- only id-protect mode allowed aggressive-only(5) -- only aggressive mode allowed.
Proposal
The index of the first IKE proposal which may be used for IKE SA negotiation with this profile.
Group
This object specifies the IKE group to use with this profile. Possible values: 1: a 768-bit MODP group 2: a 1024-bit MODP group 5: a 1536-bit MODP group 14: a 2048-bit MODP group 15: a 3072-bit MODP group 16: a 4096-bit MODP group.
Cert
The index of the certificate used for authentication in the certTable. Ignored for AuthMethod == pre_shared_key.
LocalId
The local ID used for authentication with this profile. Syntax: - X500 distinguished name: <obj-name=obj-value, obj-ID=obj-value, ...> - IPV4-Address: |123.456.789.012| with or without '|' - IPV4 Address Range: |123.456.789.012-123.456.789.013| with or without '|' - IPV4 Address Subnet: |123.456.789.012/255.255.255.0| with or without '|' or: |123.456.789.012/24| with or without '|' - Key-ID: arbitrary string: {anything} - Fully Qualified User Name (FQUN): (anything) or user@domain with mandatory '@' - Fully Qualified Domain Name (FQDN): [anything] or any name without '@' not matching any other syntax
CaCerts
Receives a comma separated list with indices (0..32767) of special certificate authority certificates accepted for this profile.
LifeTime
This object specifies an index in the ipsecLifeTimeTable with the lifetime settings to be used for IKE SA negotiation with this profile. If the lifetime pointed to by this index does not exist or is inappropriate, the default lifetime is taken. The usage of this object is deprecated, use the ikePrfLifeXxx variables directly instead.
PfsIdentity
This object specifies whether IKE SA's should be deleted immediately after a phase 2 (IPSec-) SA pair has been negotiated. The consequence of enabling this feature is that before each phase 2 negotiation there always has to be a phase 1 negotiation. Thus individual phase 2 SAs cannot be associated with one another or, respectively, if the identity of a remote peer is known to an eavesdropper for one SA, he cannot conclude that the next SA is negotiated with the same remote peer. Note: Setting this flag only makes sense if configured together with id-protect mode or RSA encryption for authentication and if the IP address of the remote peer does not allow conclusions about its identity (i.e. dynamic remote peer addresses). Possible values: true(1), -- delete phase 1 SAs false(2), -- reuse phase 1 SAs default(3) -- use value from default profile -- (false if this is the default profile).
Heartbeats
This object specifies whether heartbeats should be sent over phase 1 SAs for this profile. Possible values: none(1), -- neither send nor expect heartbeats expect(2), -- expect heartbeats send(3), -- send heartbeats both(4), -- send and expect heartbeats default(5), -- use value from default profile -- (auto if this is the default profile) auto(6), -- detect support using vendor id dpd(7), -- use DPD method for proof-of-liveliness dpd-idle(8) -- use DPD, detect dead peers even while idle.
BlockTime
This object specifies the time in seconds for which a peer is blocked for any IPSec operations after a phase 1 initiator negotiation failed. When the peer's ipsecPeerStartMode is set to 'always_up' the peer is blocked for 15 seconds even if the configured value is less than 15. Special values: -1: use settings from global profile (do not block by default) 0: do not block the peer at all.
NatT
This object specifies whether NAT-Traversal is enabled Possible values: enabled(1), -- enable Nat-Traversal disabled(2), -- disable Nat-Traversal default(3) -- use value from default profile -- (disabled, if this is the default profile).
MtuMax
The maximum MTU value allowed for ipsecPeerStatMtu. This variable affects only peers with ipsecPeerStatIpVersion 'ipv4'. Zero means use value from global profile, if this is the global profile, 1418 is assumed. Nonzero values smaller than 214 are reset to the minimum of 214.
LifeSeconds
The maximum time (in seconds) after which an SA will be deleted.
LifeKBytes
The maximum amount of data (in KB) which may be protected by an SA before it is deleted.
LifeRekeyPercent
WARNING: this object is obsolete and must not be used.
LifePolicy
This object specifies the way a lifetime proposal is handled. Possible values: loose(1), -- accept and use anything proposed strict(2), -- accept and use only what is configured notify(3), -- accept anything, if own values are smaller than what was proposed use these and send responder lifetime notification use_default_lifetime(4) -- use lifetime values from default -- profile.
Ip6MtuMax
The maximum MTU value allowed for ipsecPeerStatMtu. This variable affects only peers with ipsecPeerStatIpVersion 'ipv6' while ikePrfMtuMax affects peers with ipsecPeerStatIpVersion 'ipv4'. Zero means use value from global profile, if this is the global profile, 1398 is assumed. Nonzero values smaller than 214 are reset to the minimum of 214.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH