>> MIB - Management Information Base
>> Table: wlcPresenceProfileTable - (.1.3.6.1.4.1.272.4.61.1.39.1)
Description: Contains the global configuration of the Presence Analytics daemon.
wlcPresenceProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | OrgSecret | DisplayString | RW
.4 | CollectionInterval | INTEGER | RW
.5 | MaxElem | INTEGER | RW
.6 | DebugLevel | ENUM | RW
Index
Unique index.
AdminStatus
Activates or deactivates Presence Analytics daemon. Note that Presence Analytics must be enabled per-interface by means of 'wlcWlanIfPresence' field. Enumerations: enabled (1) disabled (2) delete (3)
OrgSecret
Customer-specific secret. This secret is used to anonymize the client MAC addresses as part of the cryptographic mechanism Length: 0 to 255
CollectionInterval
The interval in seconds to contact the collection servers. Range: 5 to 86400
MaxElem
Maximum number of probes kept in memory. When the buffer is full, the oldest entry is deleted. Range: 256 to 65535
DebugLevel
Defines the verbosity of the debugging utility for this daemon. Level 'verbose' shows the maximum amount of debugging information that can be generated by the daemon. Enumerations: quiet (1) normal (2) verbose (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH