>> MIB - Management Information Base
>> Table: certGlobals - (.1.3.6.1.4.1.272.4.26.33.1)
certGlobals
OID | Name | Type | Access
.1 | HttpProxy | DisplayString | RW
.2 | SocksServer | DisplayString | RW
.3 | MaxCacheEntries | INTEGER | RW
.4 | MaxPathLength | INTEGER | RW
.5 | MaxRestarts | INTEGER | RW
.6 | MaxCertValidity | INTEGER | RW
.7 | MaxCrlValidity | INTEGER | RW
.8 | NegCachePeriod | INTEGER | RW
.9 | PosCachePeriod | INTEGER | RW
.10 | LogLevel | INTEGER | RW
HttpProxy
This object specifies the HTTP proxy server which must be used to access the HTTP certificate servers defined. It takes either an IP-address or a fully qualified domain name. Length: 0 to 255
SocksServer
This object specifies the SOCKS server which must be used to access the HTTP and LDAP certificate servers defined. It takes either an IP-address or a fully qualified domain name. Length: 0 to 255
MaxCacheEntries
This object specifies the maximum number of certificate-cache entries allowed. Range: 64 to 8192
MaxPathLength
This object specifies the maximum number of CA certificates accepted for certificate chains from a trusted root certificate to a peer certificate. Range: 1 to 1024
MaxRestarts
This object specifies the maximum number of restarts in one certificate search.
MaxCertValidity
This object specifies the maximum validity period of a certificate in seconds. A certificate will not be considered valid for a longer period of time even if its validity field specifies a longer period.
MaxCrlValidity
This object specifies the maximum validity period of a certificate revocation list in seconds. A crl will not be considered valid for a longer period of time even if its validity field specifies a longer period.
NegCachePeriod
This object specifies the period in seconds a certificate or crl search with a negative result will be remembered. Within this time, no new search will be performed for the same item. Range: 10 to 16777216
PosCachePeriod
This object specifies the period in seconds a certificate or crl will be stored in the local certificate cache.
LogLevel
This object specifies the log level for certificate cache log events. All messages with a level higher than the value specified here are omitted, zero means no logging at all.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH