>> MIB - Management Information Base
>> Table: l2tpTunnelProfileTable - (.1.3.6.1.4.1.272.4.23.8.20.10)
Description: An entry in the l2tpTunnelProfileTable.
l2tpTunnelProfileTable
OID | Name | Type | Access
.10 | Index | INTEGER | RW
.15 | Name | DisplayString | RW
.20 | RemoteIpAddress | IpAddress | RW
.25 | RemoteIpAddressBackup | IpAddress | RW
.30 | RemoteUdpPort | INTEGER | RW
.40 | RemoteHostname | DisplayString | RW
.50 | LocalIpAddress | IpAddress | RW
.60 | LocalUdpPort | INTEGER | RW
.70 | LocalHostname | DisplayString | RW
.80 | Password | DisplayString | RW
.90 | ReceiveWindowSize | INTEGER | RW
.100 | HelloInterval | INTEGER | RW
.110 | SessionDataSequencing | ENUM | D
.120 | MinRetryTime | INTEGER | RW
.130 | MaxRetryTime | INTEGER | RW
.140 | MaxRetries | INTEGER | RW
.150 | RadiusAssignment | ENUM | RW
.160 | RadiusGroupId | INTEGER | RW
Index
The unique index for this entry.
Name
The friendly name for this entry. Length: 0 to 255
RemoteIpAddress
The main remote IP address for the tunnel. Only meaningful in LAC mode. If l2tpTunnelProfileRadiusAssignment is set to 'enabled', this object is ignored and the L2TP daemon will ask the Radius daemon to send a request for the main and backup remote IP addresses.
RemoteIpAddressBackup
The backup remote IP address for the tunnel. Only meaningful in LAC mode. If l2tpTunnelProfileRadiusAssignment is set to 'enabled', this object is ignored and the L2TP daemon will ask the Radius daemon to send a request for the main and backup remote IP addresses.
RemoteUdpPort
The remote UDP port number for the tunnel. Only meaningful in LAC mode. Range: 0 to 65535
RemoteHostname
The name of the remote host. Use an empty string for default profile. Length: 0 to 255
LocalIpAddress
The local IP address for the tunnel. If this value is set to 0, the IP address of the egress interface will be used in outgoing L2TP packets.
LocalUdpPort
The local UDP port number for the tunnel. Only meaningful in LAC mode. If this value is set to 0 (zero), the port number is allocated dynamically. Range: 0 to 65535
LocalHostname
The name of the local host. Length: 0 to 255
Password
The password used for tunnel authentication. Length: 0 to 255
ReceiveWindowSize
The received window size used by L2TP on the local side of this tunnel. Currently, the only supported value is 1. Range: 1 to 1
HelloInterval
The interval in seconds between two consecutive hello requests sent by L2TP during the tunnel life. If this object is set to 0 (zero), no hello requests are sent by L2TP on this tunnel. Range: 0 to 255
SessionDataSequencing
This object specifies if sequence numbers are used on the data channel of sessions supported by this tunnel. Additionally, if this object is set to delete (1), the entry is marked for discard. Enumerations: delete (1) disabled (2) enabled (3)
MinRetryTime
The initial interval in seconds between two consecutive attempts to send an L2TP control packet. The value of this interval is doubled with each new attempt, until the maximum value defined in l2tpTunnelProfileMaxRetryTime is reached. Range: 1 to 255
MaxRetryTime
The maximum interval in seconds between two consecutive attempts to send an L2TP control packet. Range: 8 to 255
MaxRetries
The maximum number of retries to send an L2TP control packet. The total number of attempts will be one more than this value. Range: 1 to 255
RadiusAssignment
This object enables/disables the use of Radius for requesting main and backup remote IP addresses. Only meaningful in LAC mode. Enumerations: disabled (1) enabled (2)
RadiusGroupId
Determines the logical RADIUS server group to be addressed for sending the RADIUS Access-Request messages. Only meaningful in LAC mode. See also radiusSrvGroupId. Range: 0 to 9

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH