>> MIB - Management Information Base
>> Table: ikev2RedirectTable - (.1.3.6.1.4.1.272.4.26.23.1)
Description: This object contains information for redirecting a bundle within an IKE SA.
ikev2RedirectTable
OID | Name | Type | Access
.1 | PeerIndex | INTEGER | R
.2 | NewGW | DisplayString | R
.3 | Time | Date | R
.4 | State | ENUM | R
.5 | LocalAddress | IpAddress | R
.6 | LocalMaskLen | INTEGER | R
.7 | LocalRange | IpAddress | R
.8 | LocalPort | INTEGER | R
.9 | RemoteAddress | IpAddress | R
.10 | RemoteMaskLen | INTEGER | R
.11 | RemoteRange | IpAddress | R
.12 | RemotePort | INTEGER | R
.13 | Ip6LocalAddress | InetAddressIPv6 | R
.14 | Ip6LocalMaskLen | INTEGER | R
.15 | Ip6RemoteAddress | InetAddressIPv6 | R
.16 | Ip6RemoteMaskLen | INTEGER | R
.17 | Proto | ENUM | R
.18 | RedirectedFrom | IpAddress | R
.19 | Ip6RedirectedFrom | InetAddressIPv6 | R
PeerIndex
The index of the peer which is redirected.
NewGW
The IP-address of the new gateway the peer is redirected to. This object may contain either an IP address or a domain name. Length: 0 to 255
Time
Time the redirect request was received. Range: 0 to -1
State
The current state of the received redirect request. Possible values: new(1), -- The request is newly received and not handled yet. handled(2), -- The request is already handled. Enumerations: new (1) handled (2)
LocalAddress
The local address (host or network or range start address) of the traffic selectors, source for outbound, destination for inbound.
LocalMaskLen
The local network masklen of the traffic selectors, source for outbound, destination for inbound.
LocalRange
The local address range end address of the traffic selectors, source for outbound, destination for inbound.
LocalPort
The local port of the traffic selectors, source for outbound, destination for inbound.
RemoteAddress
The remote address (host or network or range start address) of the traffic selectors source for outbound, destination for inbound.
RemoteMaskLen
The remote network masklen of the traffic selectors source for outbound, destination for inbound.
RemoteRange
The remote address range end address of the traffic selectors source for outbound, destination for inbound.
RemotePort
The remote port of the traffic selectors source for outbound, destination for inbound.
Ip6LocalAddress
The local IPv6 address (host or network or range start address) of the traffic selectors, source for outbound, destination for inbound. Length: 16 to 16
Ip6LocalMaskLen
Indicates the prefix length associated with the source (local) IPv6 address.
Ip6RemoteAddress
The remote IPv6 address (host or network or range start address) of the traffic selectors, source for outbound, destination for inbound. Length: 16 to 16
Ip6RemoteMaskLen
Indicates the prefix length associated with the destination (remote) IPv6 address.
Proto
The protocol of the traffic selectors. Enumerations: icmp (1) igmp (2) ggp (3) ipip (4) st (5) tcp (6) cbt (7) egp (8) igp (9) bbn (10) nvp (11) pup (12) argus (13) emcon (14) xnet (15) chaos (16) udp (17) mux (18) dcn (19) hmp (20) prm (21) xns (22) trunk1 (23) trunk2 (24) leaf1 (25) leaf2 (26) rdp (27) irtp (28) isotp4 (29) netblt (30) mfe (31) merit (32) sep (33) pc3 (34) idpr (35) xtp (36) ddp (37) idprc (38) tp (39) il (40) ipv6 (41) sdrp (42) ipv6route (43) ipv6frag (44) idrp (45) rsvp (46) gre (47) mhrp (48) bna (49) esp (50) ah (51) inlsp (52) swipe (53) narp (54) mobile (55) tlsp (56) skip (57) ipv6icmp (58) ipv6nonxt (59) ipv6opts (60) ipproto-61 (61) cftp (62) local (63) sat (64) kryptolan (65) rvd (66) ippc (67) distfs (68) satmon (69) visa (70) ipcv (71) cpnx (72) cphb (73) wsn (74) pvp (75) brsatmon (76) sunnd (77) wbmon (78) wbexpak (79) isoip (80) vmtp (81) securevmtp (82) vines (83) ttp (84) nsfnet (85) dgp (86) tcf (87) eigrp (88) ospfigp (89) sprite (90) larp (91) mtp (92) ax25 (93) ipwip (94) micp (95) scc (96) etherip (97) encap (98) encrypt (99) gmtp (100) ifmp (101) pnni (102) pim (103) aris (104) scps (105) qnx (106) an (107) ippcp (108) snp (109) compaq (110) ipxip (111) vrrp (112) pgm (113) hop0 (114) l2tp (115) ipproto-116 (116) ipproto-117 (117) ipproto-118 (118) ipproto-119 (119) ipproto-120 (120) ipproto-121 (121) ipproto-122 (122) ipproto-123 (123) ipproto-124 (124) ipproto-125 (125) ipproto-126 (126) ipproto-127 (127) ipproto-128 (128) ipproto-129 (129) ipproto-130 (130) ipproto-131 (131) ipproto-132 (132) ipproto-133 (133) ipproto-134 (134) ipproto-135 (135) ipproto-136 (136) ipproto-137 (137) ipproto-138 (138) ipproto-139 (139) ipproto-140 (140) ipproto-141 (141) ipproto-142 (142) ipproto-143 (143) ipproto-144 (144) ipproto-145 (145) ipproto-146 (146) ipproto-147 (147) ipproto-148 (148) ipproto-149 (149) ipproto-150 (150) ipproto-151 (151) ipproto-152 (152) ipproto-153 (153) ipproto-154 (154) ipproto-155 (155) ipproto-156 (156) ipproto-157 (157) ipproto-158 (158) ipproto-159 (159) ipproto-160 (160) ipproto-161 (161) ipproto-162 (162) ipproto-163 (163) ipproto-164 (164) ipproto-165 (165) ipproto-166 (166) ipproto-167 (167) ipproto-168 (168) ipproto-169 (169) ipproto-170 (170) ipproto-171 (171) ipproto-172 (172) ipproto-173 (173) ipproto-174 (174) ipproto-175 (175) ipproto-176 (176) ipproto-177 (177) ipproto-178 (178) ipproto-179 (179) ipproto-180 (180) ipproto-181 (181) ipproto-182 (182) ipproto-183 (183) ipproto-184 (184) ipproto-185 (185) ipproto-186 (186) ipproto-187 (187) ipproto-188 (188) ipproto-189 (189) ipproto-190 (190) ipproto-191 (191) ipproto-192 (192) ipproto-193 (193) ipproto-194 (194) ipproto-195 (195) ipproto-196 (196) ipproto-197 (197) ipproto-198 (198) ipproto-199 (199) ipproto-200 (200) ipproto-201 (201) ipproto-202 (202) ipproto-203 (203) ipproto-204 (204) ipproto-205 (205) ipproto-206 (206) ipproto-207 (207) ipproto-208 (208) ipproto-209 (209) ipproto-210 (210) ipproto-211 (211) ipproto-212 (212) ipproto-213 (213) ipproto-214 (214) ipproto-215 (215) ipproto-216 (216) ipproto-217 (217) ipproto-218 (218) ipproto-219 (219) ipproto-220 (220) ipproto-221 (221) ipproto-222 (222) ipproto-223 (223) ipproto-224 (224) ipproto-225 (225) ipproto-226 (226) ipproto-227 (227) ipproto-228 (228) ipproto-229 (229) ipproto-230 (230) ipproto-231 (231) ipproto-232 (232) ipproto-233 (233) ipproto-234 (234) ipproto-235 (235) ipproto-236 (236) ipproto-237 (237) ipproto-238 (238) ipproto-239 (239) ipproto-240 (240) ipproto-241 (241) ipproto-242 (242) ipproto-243 (243) ipproto-244 (244) ipproto-245 (245) ipproto-246 (246) ipproto-247 (247) ipproto-248 (248) ipproto-249 (249) ipproto-250 (250) ipproto-251 (251) ipproto-252 (252) ipproto-253 (253) ipproto-254 (254) dont-verify (255)
RedirectedFrom
The IP address of the original gateway from which we got redirected.
Ip6RedirectedFrom
The IPv6 address of the original gateway from which we got redirected. Length: 16 to 16

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH