>> MIB - Management Information Base
>> Table: systemPhoneFwuServerUpdTable - (.1.3.6.1.4.1.272.4.64.5.4.1)
Description: This table contains URL informations for firmware update of system phones.
systemPhoneFwuServerUpdTable
OID | Name | Type | Access
.1 | DevClass | ENUM | R
.2 | DevType | ENUM | R
.3 | PathDefault | DisplayString | R
.4 | Path | DisplayString | RW
DevClass
The device class (company) the system phone belongs to. Enumerations: elmeg (1) unify (2) gigaset (3)
DevType
The specific device type of the system phone. Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145) ip120 (160) ip140 (161) dect150 (162) dect200-b (163) dect200-m (164) ip130 (165) ip620 (166) dect210 (167) ip630 (168) ip640 (169) ip680 (171) de310-ip-pro (176) de410-ip-pro (177) de700-ip-pro (178) de900-ip-pro (179) n510-ip-pro (180) n720-ip-pro (181) n720-dm-pro (182) maxwell-basic (183) n870-ip-pro (184) maxwell-3 (185) maxwell-4 (186) maxwell-10 (188)
PathDefault
This is the default URL used for a specific system phone FW update. It is set by the FW update server process and should be used if no systemPhoneFwuServerUpdPath is defined. Length: 0 to 255
Path
This is the configured URL used for a specific system phone FW update. It overrides the value set in systemPhoneFwuServerUpdPathDefault. If the string is empty then the systemPhoneFwuServerUpdPathDefault is used. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH