>> MIB - Management Information Base
>> Table: wlanBridgeLinkTable - (.1.3.6.1.4.1.272.4.46.32.1)
Description: Contains the configuration of WLAN bridge links (WBL)
wlanBridgeLinkTable
OID | Name | Type | Access
.1 | WlanIf | INTEGER | RW
.2 | IfIndex | INTEGER | R
.3 | Id | DisplayString | RW
.4 | PassPhrase | OCTET STRING | RW
.5 | Role | ENUM | D
WlanIf
Radio index the WLAN bridge link belongs to.
IfIndex
System generated unique WLAN bridge link index.
Id
This attribute reflects the Service Set ID.
PassPhrase
Pass phrase used for authentication.
Role
Each WBL configuration has exact one WBL master and at least one WBL slave. The WBL master is like an AP where all WBL slaves can connect.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH