>> MIB - Management Information Base
>> Table: mpsSysUserConfig - (.1.3.6.1.4.1.272.4.53.1.5)
mpsSysUserConfig
OID | Name | Type | Access
.1 | PIN | DisplayString | RW
.2 | ExternPIN | DisplayString | RW
.3 | Facilities | BITS | RW
.4 | CoS | ENUM | RW
.5 | PBXMode | ENUM | RW
.6 | NightGroupMode | INTEGER | RW
.7 | NightDoorIntercomMode | INTEGER | RW
.8 | NightTrunkMode | INTEGER | RW
.9 | NightExtensionMode | INTEGER | RW
.10 | NightGlobalReRouteMode | INTEGER | RW
.11 | DayGlobalReRouteMode | INTEGER | RW
.12 | NightAlarmInputMode | INTEGER | RW
PIN
This variable contains the system PIN code for configuration. 'none' = inactive (can not be dialed). Length: 4 to 4
ExternPIN
This variable contains the system PIN code for remote control. Length: 6 to 6
Facilities
System facilities. (1) enabled or (0) disabled: remoteConfig : Remote switching/ remote control. remoteAccess : Remote access. callRecordPrinting: Print call data records. Enumerations: remoteConfig (0) remoteAccess (1) callRecordPrinting (2)
CoS
This variable contains the current Class Of Service mode. Enumerations: standard (1)
PBXMode
This variable contains the current PBX mode. Enumerations: day (1) night (2)
NightGroupMode
This variable contains the active group mode when the mpsSysConfigPBXMode = night. 0 = night mode for groups is off, individual settings used (day). Range: 0 to 4
NightDoorIntercomMode
This variable contains the active DoorIntercom mode when variable mpsSysConfigPBXMode is set to night. Value 0 means night mode for door intercom units is off, individual settings used (day). Range: 0 to 4
NightTrunkMode
This variable contains the active trunk mode when variable mpsSysConfigPBXMode is set to night and mpsTrunkNumberTarget is set to re-route. 0 = night mode for trunk rerouting is off, individual settings used (day). Range: 0 to 4
NightExtensionMode
This variable contains the active extension mode when variable mpsSysConfigPBXMode is set to night and rerouting is active. 0 = night mode for extension is off, individual settings used (day). Range: 0 to 4
NightGlobalReRouteMode
This variable contains the active reroute mode when variable mpsSysConfigPBXMode is set to night and global rerouting is available. 0 = night mode for global rerouting is off, individual settings used (day). Range: 0 to 4
DayGlobalReRouteMode
This variable contains the active global reroute mode when variable mpsSysConfigPBXMode is set to day and global rerouting is available. Range: 1 to 4
NightAlarmInputMode
This variable contains the active alarm input mode when variable mpsSysConfigPBXMode is set to night. 0 = night mode for alarm input is off, so use the individual settings. Range: 0 to 2

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH