>> MIB - Management Information Base
>> Table: sysPedTemperature - (.1.3.6.1.4.1.272.4.17.6.2)
sysPedTemperature
OID | Name | Type | Access
.1 | Current | INTEGER | R
.2 | Max | INTEGER | R
.3 | MaxTime | Date | R
.4 | Min | INTEGER | R
.5 | MinTime | Date | R
.6 | UpdatePeriod | Unsigned32 | RW
.7 | LowerThreshold | INTEGER | RW
.8 | UpperThreshold | INTEGER | RW
.9 | Alarm | ENUM | R
Current
Temperature during the last measurement time. Range: -55 to 150
Max
Maximum observed temperature. Range: -55 to 150
MaxTime
Point in time the maximum temperature was observed. Range: 0 to -1
Min
Minimum observed temperature. Range: -55 to 150
MinTime
Point in time the minimum temperature was observed. Range: 0 to -1
UpdatePeriod
Measurement interval of temperature update in seconds. 0: Disable measurements.
LowerThreshold
Minimal allowed temperature. If temperature falls below this threshold, a syslog message is generated. Range: -55 to 125
UpperThreshold
Maximal allowed temperature. If temperature raises above this threshold, a syslog message is generated. Range: -55 to 125
Alarm
Indicates if the defined temperature thresholds are violated. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH