>> MIB - Management Information Base
>> Table: mpsHotelWakeUp - (.1.3.6.1.4.1.272.4.53.16.2)
mpsHotelWakeUp
OID | Name | Type | Access
.1 | Duration | INTEGER | RW
.2 | PlaybackNumber | INTEGER | RW
.3 | RepeatTime | INTEGER | RW
.4 | AnnDefault | ENUM | RW
.5 | NumberOfRepetition | INTEGER | RW
.6 | AnnDefaultFileDirectory | DisplayString | RW
.7 | AnnDefaultDefaultVariant | INTEGER | RW
Duration
This variable contains the duration of the wakeUp announcement in seconds. Range: 1 to 99
PlaybackNumber
This variable contains number of play-back loops. Range: 1 to 5
RepeatTime
This variable contains the time delay in minutes before repeating the wakeUp call if not connected. Range: 0 to 5
AnnDefault
This variable contains the selected music on hold (MoH) that the wakeUp party hears, if no special wakeUp announcement is selected for the wakeUp party (default). Possible values are: file: variable mpsHotelWakeUpAnnDefaultFileDirectory specifies directory to contain sound file default: variable mpsHotelWakeUpAnnDefaultDefaultVariant specifies the variant whose default is to be used (default) Enumerations: file (54) default (55)
NumberOfRepetition
This variable contains number of wake-up-call repetitions. Range: 0 to 5
AnnDefaultFileDirectory
Name of directory (on flash medium) which contains file to be used for music on hold. This variable references the entry in mpsWaveFile table where variable mpsWaveFileDirectory has identical content. If there should be multiple entrys with the same content for some reason an arbitrary entry is chosen. This entry is only valid if variable mpsHotelWakeUpAnnDefault is set to value file. Default value is the empty string. Length: 0 to 255
AnnDefaultDefaultVariant
This variable specifies the chosen default variant if variable mpsHotelWakeUpAnnDefault is set to value default. Default value for that variable is 1. Range: 1 to 2

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH