>> MIB - Management Information Base
>> Table: pptpCtlConnTable - (.1.3.6.1.4.1.272.4.23.2.1)
Description: The pptpCtlConnTable displays all currently active PPTP dontrol connections Only the system can add or remove entries to this table. Creating entries: Entries are added when an outgoing or incoming TCP connection (port 1723) is established. Deleting entries: Entries are removed once the respective PPTP control connection is disconnected.
pptpCtlConnTable
OID | Name | Type | Access
.1 | Originator | ENUM | R
.2 | Age | TimeTicks | R
.3 | State | ENUM | D
.4 | RemoteIpAddress | IpAddress | R
.5 | LocalIpAddress | IpAddress | R
.6 | Version | INTEGER | R
.7 | Host | DisplayString | R
.8 | Vendor | DisplayString | R
.9 | FirmRev | INTEGER | R
.10 | MaxChan | INTEGER | R
.11 | OutgoingCalls | INTEGER | R
.12 | IncomingCalls | INTEGER | R
.13 | OutgoingFails | INTEGER | R
.14 | IncomingFails | INTEGER | R
.15 | EchoReqSent | INTEGER | R
.16 | EchoReqRcvd | INTEGER | R
.17 | EchoRepSent | INTEGER | R
.18 | EchoRepRcvd | INTEGER | R
.19 | EchoReqPending | INTEGER | R
Originator
The originator of the PPTP control connection. Enumerations: local (1) remote (2)
Age
The age of the PPTP control connection. The format is in hh:mm:ss.00.
State
The state of the PPTP control connection according RFC 2637. Enumerations: idle (1) wait-ctl-reply (2) established (3) wait-stop-reply (4) close (5) delete (6)
RemoteIpAddress
The IP address of the remote PPTP tunnel endpoint.
LocalIpAddress
The IP address of the local PPTP tunnel endpoint.
Version
This variable contains the negotiated PPTP version.
Host
DNS name of the issuing PAC or PNS. Length: 0 to 255
Vendor
Vendor specific string describing the type of PAC or PNS being used on remote side. Length: 0 to 255
FirmRev
This variable contains the firmware revision number of the issuing PAC or PNS.
MaxChan
The maximum number of individual PPP sessions for this PPTP control connection.
OutgoingCalls
The number of currently established individual outgoing PPP sessions for this PPTP control connection.
IncomingCalls
The number of currently established individual incoming PPP sessions for this PPTP control connection.
OutgoingFails
The number of failed outgoing PPP sessions for this PPTP control connection.
IncomingFails
The number of failed incoming PPP sessions for this PPTP control connection.
EchoReqSent
The number of PPTP Echo-Request packets sent for this PPTP control connection.
EchoReqRcvd
The number of PPTP Echo-Request packets received for this PPTP control connection.
EchoRepSent
The number of PPTP Echo-Reply packets sent for this PPTP control connection.
EchoRepRcvd
The number of PPTP Echo-Reply packets received for this PPTP control connection.
EchoReqPending
The number of currently unanswered PPTP Echo-Request packets for this PPTP control connection.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH