>> MIB - Management Information Base
>> Table: ipRTPSessionTable - (.1.3.6.1.4.1.272.4.5.58.1)
Description: Contains the description of a RTP Stream Session
ipRTPSessionTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | SourceAddress | IpAddress | R
.3 | SourcePort | INTEGER | R
.4 | SourceIf | INTEGER | R
.5 | DestinationAddress | IpAddress | R
.6 | DestinationPort | INTEGER | R
.7 | DestinationIf | INTEGER | R
.8 | SessionIdent | INTEGER | R
.9 | SessionState | ENUM | R
.10 | SessionSSRC | HexValue | R
.11 | SessionPayload | INTEGER | R
.12 | SessionPackets | INTEGER | R
.13 | SessionManage | ENUM | R
.14 | SourceInetAddressType | ENUM | R
.15 | SourceInetAddress | InetAddress | R
.16 | DestinationInetAddressType | ENUM | R
.17 | DestinationInetAddress | InetAddress | R
Index
Index of the RTP Session
SourceAddress
Source Address of the RTP Session
SourcePort
Source Port of the RTP Session Range: 0 to 65535
SourceIf
Source Interface of the RTP Session
DestinationAddress
Destination Address of the RTP Session
DestinationPort
Destination Port of the RTP Session Range: 0 to 65535
DestinationIf
Destination Interface of the RTP Session
SessionIdent
Identifier of the RTP Session
SessionState
State of the RTP Session Enumerations: new (1) init (2) check (3) up (4) delete (8)
SessionSSRC
Unique RTP Session Identifier (SSRC field in RTP header) Range: 0 to -1
SessionPayload
Payload Type of the RTP Stream (alaw, ulaw...) Range: 0 to 255
SessionPackets
Current Packets of the RTP Stream (session_handler only)
SessionManage
Creator of the RTP entry Enumerations: session-handler (1) media-gateway (2) application-gateway (3)
SourceInetAddressType
The Address Type of the Source Address Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
SourceInetAddress
Source Address of the RTP Session Length: 0 to 255
DestinationInetAddressType
The Address Type of the Destination Address Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
DestinationInetAddress
Destination Address of the RTP Session Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH