>> MIB - Management Information Base
>> Table: trempAdmin - (.1.3.6.1.4.1.272.4.99.1.1)
trempAdmin
OID | Name | Type | Access
.1 | Status | ENUM | RW
.2 | OperStatus | ENUM | R
.3 | Server | DisplayString | RW
.4 | QueryInterval | INTEGER | RW
.5 | PurgeSecurity | ENUM | RW
.6 | DebugLevel | ENUM | RW
.7 | StartupTimer | INTEGER | RW
Status
Activate or deactivate the TREMP client. Enumerations: enabled (1) disabled (2)
OperStatus
Operational status of the TREMP client. Enumerations: enabled (1) disabled (2) managed (3) idle (4) startup (5)
Server
The address of the TREMP server. This object can start with the scheme 'http://' or 'https://'. The address may contain either an IP address or a domain name and can be followed by the port separated by a colon. Length: 0 to 255
QueryInterval
The interval in seconds to query the TREMP server for new tasks. Range: 5 to 3600
PurgeSecurity
Removes security information from the system. Enumerations: enabled (1) disabled (2)
DebugLevel
Defines the verbosity of the debugging utility for this daemon. The 'verbose' level shows the maximum amount of debugging information that can be generated by the daemon. Enumerations: normal (1) verbose (2) quiet (3)
StartupTimer
Defines the amount of time that the daemon will wait on startup before running. Range: 0 to 3600

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH