>> MIB - Management Information Base
>> Table: mpsExtensionABTable - (.1.3.6.1.4.1.272.4.53.6.5.1)
Description: This table contains the additional information of the analog extension.
mpsExtensionABTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | Mode | ENUM | RW
.3 | GatewayNumber | INTEGER | RW
.4 | DialingType | ENUM | RW
.5 | ChargePulse | ENUM | RW
.6 | Clip | ENUM | RW
.7 | ClipOffHook | ENUM | RW
.8 | Cnip | ENUM | RW
.9 | FlashTime | ENUM | RW
.10 | DoorIntercom | DoorIntercomIndexOrZero | RW
.11 | DoorIntercomTimer | INTEGER | RW
.12 | AdminStatus | ENUM | D
Index
A unique value for additional analog extension settings. Range: 1 to 65535
Mode
You can configure each analog port to accept a different terminal device. Additional settings or special functions may be required depending on the type of terminal device. Terminal device types which require special functions / applications can be set at some analog connections. Set to delete, to discard the whole entry. Enumerations: none (1) telephone (2) fax (3) answering-machine (4) modem (5) multi-port (6) moh (7) tfe-123d12 (8) tfe-other (9) tfe-doorline (10) announcement (11) voice-mail-system (12) alarm-line (13) tfe-adapter (14) moh-anouncement (15) tfe-123d12-4bells (16) tfe-others-4bells (17) gateway (18)
GatewayNumber
This variable contains the gateway number, if mpsExtensionABMode=gateway.
DialingType
Type of dialling, DTMF and pulse dialing. Enumerations: none (1) mfv (2) iwv (3)
ChargePulse
If your analog terminal devices support the display of cost and charge information you can set the transmission of charge pulses at the corresponding connections. Enumerations: true (1) false (2)
Clip
Number display (CLIP). Enumerations: none (1) mfv (2) dtmf (3)
ClipOffHook
Number display (CLIP off Hook). Enumerations: true (1) false (2)
Cnip
Name display (CNIP). Enumerations: true (1) false (2)
FlashTime
This variable contains the analogue flash time in milliseconds. Enumerations: m100 (1) m200 (2) m300 (3) m400 (4) m500 (5) m600 (6) m700 (7) m800 (8) m900 (9) m1000 (10)
DoorIntercom
This variable contains the number of the door intercom. Range: 0 to 10
DoorIntercomTimer
This variable contains the length of timer in seconds for open door.
AdminStatus
Jsut for delete. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH