>> MIB - Management Information Base
>> Table: igmpACLTable - (.1.3.6.1.4.1.272.4.5.51.7.1)
Description: An entry (conceptual row) representing an ACL rule.
igmpACLTable
OID | Name | Type | Access
.1 | Order | Integer32 | RC
.2 | Status | ENUM | D
.3 | Action | ENUM | RC
.4 | IfIndex | InterfaceIndex | RC
.5 | SenderAddress | IpAddress | RC
.6 | SenderNetmask | IpAddress | RC
.7 | GroupAddress | IpAddress | RC
.8 | GroupNetmask | IpAddress | RC
.9 | Type | ENUM | RC
Order
The order of this entry.
Status
The status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)
Action
Status of this rule. Enumerations: accept (1) deny (2)
IfIndex
The incoming interface for which this rule applies. Range: 1 to 2147483647
SenderAddress
The originator of the packet for which this rule applies.
SenderNetmask
The netmask of the originator for which this rule applies.
GroupAddress
The address (combined with igmpACLGroupMask) which specifies a multicast group.
GroupNetmask
The netmask (combined with igmpACLGroup) which specifies a multicast group.
Type
The type for which this rule applies, either IGMP reporting or incoming mulicast traffic. Enumerations: report (1) traffic (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH