>> MIB - Management Information Base
>> Table: ipSif - (.1.3.6.1.4.1.272.4.5.37)
ipSif
OID | Name | Type | Access
.1 | AdminStatus | ENUM | RW
.2 | LocalFilter | ENUM | RW
.3 | InterfaceFilter | ENUM | RW
.4 | Sysloglevel | ENUM | RW
.5 | UdpTimeout | INTEGER | RW
.6 | TcpTimeout | INTEGER | RW
.7 | PPTPTimeout | INTEGER | RW
.8 | DefaultTimeout | INTEGER | RW
.9 | MaxSessions | INTEGER | RW
.14 | MaxRejectEntries | INTEGER | RW
.15 | MaxRejectTtl | INTEGER | RW
.16 | InterfaceAliasAutoCreate | ENUM | RW
.17 | UdpStunPort | INTEGER | RW
.18 | UdpSipPort | INTEGER | RW
.19 | UdpSipTimeout | INTEGER | RW
AdminStatus
Enable or disable Stateful Inspection Firewall. If set to reset(3) all ipSifAliasTable and ipSifAliasAddressTable entries will be deleted and partly recreated due to the SIF startup policy, ipSifAdminStatus is set to disable(2) afterwards. Enumerations: enable (1) disable (2) reset (3)
LocalFilter
Enable or disable filtering on local requests Enumerations: enable (1) disable (2)
InterfaceFilter
Enable or disable filtering on same Interface packets Enumerations: enable (1) disable (2)
Sysloglevel
Levels for less or more Informations in the Syslog, verbose : display all Sif Activity deny : display only rejects, ignore accept : display only accpts none : disable Syslogs Enumerations: deny (1) accept (2) verbose (3) none (4)
UdpTimeout
Timeout on inactive UDP Session Range: 30 to 86400
TcpTimeout
Timeout on inactive TCP Session Range: 30 to 86400
PPTPTimeout
Timeout on inactive PPTP Session Range: 30 to 86400
DefaultTimeout
Timeout on all other ip Sessions Range: 30 to 86400
MaxSessions
Maximum number of monitored sessions Range: 0 to 1000000
MaxRejectEntries
Maximum number of ipSifRejectTable entries Range: 0 to 10000
MaxRejectTtl
Maximum time to live of the ipSifRejectTable entries in seconds Range: 5 to 86400
InterfaceAliasAutoCreate
Enable or disable automatic creation of interface aliases (see ipSifAliasAddressTable) due to created MPR interfaces visible in ifTable. Enumerations: enable (1) disable (2)
UdpStunPort
Optional UDP port number for STUN, if addressed by IP packets from address X and from UDP port Y it will trigger creation of an implicit allow rule for all UDP packets addressed to X:Y. Range: 0 to 65535
UdpSipPort
Optional UDP port number for SIP, in case of matching UDP packets it triggers consideration of the ipSifUdpSipTimeout value for all associated sessions. Range: 0 to 65535
UdpSipTimeout
Timeout for inactive SIP sessions (identification works via optional ipSifUdpSipPort setting). Range: 30 to 86400

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH