>> MIB - Management Information Base
>> Table: layer25WildcardTable - (.1.3.6.1.4.1.272.4.56.3.1)
Description: Each entry contains a unique layer-2.5 interface instance.
layer25WildcardTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Mode | ENUM | RW
.3 | MacAddr | MacAddress | RW
.4 | Transparent | ENUM | RW
IfIndex
The interface index identifying the layer-2.5 interface instance.
Mode
The layer-2.5 wildcard mode determines the handling of non-IP/ARP frames. With wildcard mode equal to none(0), any unicast non-IP/ARP frames get dropped. With wildcard mode equal to static(1), the wildcard MAC address is writable and any unicast non-IP/ARP frames will be converted using that MAC address. With wildcard mode first(2), the source MAC address of the first frame received on the mobile LAN determines the wildcard MAC address - independent of the protocol type. With wildcard mode last(3), the source MAC address of the last non-IP/ARP frame received determines the wildcard MAC address. The wildcard mode reset(4) resets the learn table and in case of wildcard mode first(2) and last(3) also the wildcard MAC address. Enumerations: none (0) static (1) first (2) last (3) reset (4)
MacAddr
The MAC address used for translating non-IP/ARP frames. Length: 6 to 6
Transparent
The transparent value determines if the physical MAC address of the layer-2.5 interface is updated with the wildcard MAC address. This option can be enabled only if the wilcard mode is set to either static(1) or first(2). Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH